519B-A239单颗复古外辅光灯说明书
I. Definition of Display Panel and Keys
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Menu up and down confirmation
Menu key: select function
Up arrow: parameter increment
Down arrow: decreasing parameter
Confirm key: OK and save.

Second, the menu function
Press the menu key after powering on and turning on, and the menu menu will appear in turn; Press the up or down key to modify the function parameters, and press the Enter key to save the current function and parameters (with power-off memory after saving).
Menu menu:
	A001
	
	A512
	Set the address code, modify the address code (A001~A512) up or down, and confirm to save.

	CH04
	
	CH147
	Switch the three channels CH04, CH10 and CH55 up or down, and confirm to save. Default CH10

	M000
	
	M127
	Effect mode, switch the built-in effect up or down, and confirm to save.

	S000
	
	S255
	Modify the running speed of hexagon built-in effect up or down (S000~ S255), and confirm to save.

	Soud
	
	Soud
	Voice control mode.

	R255
	
	R000
	R Dimming the red light bulb, modify the brightness of the red light bulb up or down (R000~ R255), and press the Enter key to save.

	G255
	
	G000
	G dim the green light bulb, modify the brightness of the green light bulb up or down (G000~ G255), and press the Enter key to save.

	B255
	
	B000
	B Dim the blue light bulb, modify the brightness of the blue light bulb up or down (B000~ B255), and press the Enter key to save.

	W255
	
	W000
	W Monochrome lamp brightness, modify the monochromatic lamp brightness up or down (W000~W255), and press the Enter key to save.

	T000
	
	
	Display the temperature, such as T045, indicating that the current lamp temperature is 45℃.



Third, master-slave control
Two or more identical lamps are connected by DMX three-core signal lines, all lamps are set to any address code A001~A512, and any one is set as the master, while other lamps are slaves, and all slave displays do not flicker; When the master adjusts the effects of gradual change, pulse change, jump, voice control and self-walking, all slaves synchronize the effects of gradual change, pulse change, jump, voice control and self-walking.
Special attention: 1. Only one host can be set for a group of lamps. If there are multiple hosts, all lamps will flash without synchronization.
2. All lamps and lanterns must be used when the DMX512 console is closed.


Fourth, the factory settings
Press the menu key for 3 seconds to enter the factory setting when any address code is A001~A512. Factory settings mainly include the functions of each output power of lamps and lanterns, fan setting mode, setting temperature protection point and sending parameters. The factory sets any mode and presses the menu button for 3 seconds to exit.
Factory Settings Table:
	R255
	
	R020
	R red light bulb current setting, modify the hexagonal red light bulb current (R020-R255) up or down, and confirm to save.

	G255
	
	G020
	G green light bulb current setting, modify the hexagonal green light bulb current (G020-G255) up or down, and confirm to save.

	B255
	
	B020
	B blue light bulb current setting, modify the hexagonal blue light bulb current up or down (B020-B255), and confirm to save.

	W255
	
	W020
	W monochrome lamp current setting, modify the monochrome lamp current setting up or down (W020~W255), and press the Enter key to save.

	FAN1
	
	FAN0
	Fan setting: start the fan as soon as the FAN0 light bulb lights up, and start the fan as soon as the FAN1 reaches the set temperature protection point, and press the Enter key to save.

	T040
	
	T-105
	Set the temperature protection point, modify the parameters (40℃~75℃) up or down, and press the Enter key to save.

	Send
	
	Send
	Send the factory setting parameters of this machine up or down to all other lamps with three-core signal lines connected in parallel; Confirm the sending parameters and press the menu button for 3 seconds.
Exit, deny the parameter and press the confirm key to cancel sending.



V. DMX512 console
After electrifying, the address codes of all lamps and lanterns are set, and all lamps and lanterns are connected to the DMX512 console in parallel with three-core signal lines, and the address codes will stop flashing, indicating that the DMX512 console signal has been sent to the lamps and lanterns. According to each channel description, the DMX512 console is used to control related functions.


CH4 channel description:
	passage
	Channel value
	fundamental function

	one
	000-255
	Linear dimming of red lamp beads

	2
	000-255
	Linear dimming of green lamp beads

	three
	000-255
	Linear dimming of blue lamp beads

	four
	000-255
	Linear dimming of white lamp beads






CH10 channel description:
	passage
	Channel value
	fundamental function

	one
	000-255
	Total dimming

	2
	000-255
	stroboscopic

	three
	000-255
	white light

	four
	000-255
	red

	five
	000-255
	green

	six
	000-255
	blue

	seven
	000-255
	model

	eight
	000-255
	speed

	nine
	000-255
	background color

	10
	000-255
	Background tone light




CH55 channel description:
	Channel value
	Mode code
	effect

	one
	000-255
	Linear dimming of the first group of red lamp beads

	2
	000-255
	Group 1 Linear Dimming of Green Lamp Beads

	three
	000-255
	Linear dimming of the first group of blue lamp beads

	four
	000-255
	Group 2 Linear Dimming of Red Lamp Beads

	five
	000-255
	Group 2 Linear Dimming of Green Lamp Beads

	six
	000-255
	Linear dimming of the second group of blue lamp beads

	…
	…
	… …

	fifty-two
	000-255
	Group 18 Linear Dimming of Red Lamp Beads

	53
	000-255
	Group 18 Linear Dimming of Green Lamp Beads

	54
	000-255
	Group 18 Linear Dimming of Blue Lamp Beads

	55
	000-255
	Linear dimming of white lamp beads





VI. Technical parameters:
[bookmark: OLE_LINK5]Voltage: AC100~220V 50/60HZ
Power: 72*0.25W(18W)+ 60W
Lamp beads: 72 5050 tri-color LED lamp beads+long white light lamp beads
Control mode: DMX512, self-propelled, master-slave, voice control and RDM function.
Channels: CH04, CH10 and CH55
Dimming: 32bit 0~100% linear dimming
Features: dyeing+flash+auxiliary light
Working temperature: -30 ~50℃
Strobe frequency: 1~30HZ
Appearance: metal, black
Connection mode: DMX512 input/output/power input/output.
IP grade: IP20
Size: 20*13*18 CM
Weight: 1.6KG
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