36颗钻石矩阵说明书
First, the display panel
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Menu up and down confirmation
Key definition:
Menu key: select function
Up arrow: parameter increment
Down arrow: decreasing parameter
Confirm key: OK and save.
Second, the menu function
Press the menu key after powering on and turning on, and the menu menu will appear in turn; Press the up or down key to modify the function parameters, and press the Enter key to save the current function and parameters (with power-off memory after saving).
Menu menu:
	A001
	
	A512
	Modify the address code (A001~A512) up or down, and press the Enter key to save. A001 is the default.

	C004
	
	C144
	Modify channels C004, C12 and C144 up or down, and confirm to save. The default is CH12.

	M000
	
	M096
	Modify the built-in effect (M000~M096) up or down, and press OK to save. The default value is M000.

	S000
	
	S255
	Modify the running speed of the built-in effect up or down (S000~S255), press the Enter key to save, and the default value is S010.

	R255
	
	R000
	Modify the brightness of the red light bulb (R000~ R255) up or down, and press the Enter key to save. R255 is the default.

	G255
	
	G000
	Modify the brightness of the green light bulb (G000~G255) up or down, and press the Enter key to save. The default value is G255.

	B255
	
	B000
	Modify the brightness of the blue light bulb (B000~ B255) up or down, and press the Enter key to save. B255 is the default.

	W255
	
	W000
	Modify the brightness of the white light bulb (B000~ B255) up or down, and press the Enter key to save. B255 is the default.

	T000
	
	
	Display the temperature, such as T045, indicating that the current lamp temperature is 45℃; 10K thermistor display T000 is not installed.



Third, the factory settings
In case of any address code from A001~A512, press the menu key for 5 seconds to enter the factory setting. The factory settings mainly include the functions of lamp output power, fan setting mode, setting temperature protection point and sending parameters. Press the menu button for 5 seconds to exit any mode set by the factory.
Factory Settings Table:
	R255
	
	R032
	Modify the red bulb current (R032~ R255) up or down, and press the Enter key to save. R220 is the default.

	G255
	
	G032
	Modify the green bulb current (G032~G255) up or down, and press the Enter key to save. The default value is G220.

	B255
	
	B032
	Modify the blue bulb current (B032~ B255) up or down, and press the Enter key to save. B220 is the default.

	W255
	
	W032
	Modify the white bulb current (w032~ w255) up or down, and press the Enter key to save. The default value is w220.

	Dir0
	
	Dir7
	Modify the direction of running water (d0~ d7) up or down, and confirm to save. d0 is the default.

	FAN0
	
	FAN1
	Fan setting: start the fan when the light bulb of FAN0 is on, and start the fan when the temperature of FAN1 reaches 40 degrees. Press the Enter key to save.

	T040
	
	T070
	Set the temperature protection point, modify the parameters (40℃~70℃) up or down, and press the Enter key to save. The default value is T065.

	Send
	
	Send
	Send the factory setting parameters of this machine up or down to all other lamps with three-core signal lines connected in parallel; Press the menu button for 5 seconds to confirm the sending parameters, and press the confirm button to cancel the sending if the parameters are denied.


Fourth, master-slave control
Two or more identical lamps are connected by DMX three-core signal lines, all lamps are set to any address code A001~A512, and any one is set as the master, while other lamps are slaves, and all slave displays do not flicker; When the master adjusts the gradient, pulse change, voice control and self-propelled effect, all slaves synchronize the gradient, pulse change, voice control and self-propelled effect.
Special attention: 1. Only one host can be set for a group of lamps. If there are multiple hosts, all lamps will flash without synchronization.
2. All lamps and lanterns must be used when the DMX512 console is closed.
V. DMX512 console
Set the address codes of all lamps and lanterns after power-on, and then connect all lamps and lanterns to DMX512 console in parallel with three-core signal lines. The address codes will stop flashing, indicating that DMX512 console signals have been sent to lamps and lanterns, and use DMX512 console to control related functions according to the channel table.
CH04 Channel Table Description:
	passage
	Channel value
	Basic function of channel

	one
	000-255
	R red lamp bead linear dimming

	2
	000-255
	G linear dimming of green lamp beads

	three
	000-255
	B linear dimming of blue lamp beads

	four
	000-255
	W white lamp bead linear dimming


CH12 Channel Table Description:
	passage
	Channel value
	Basic function of channel

	one
	000-255
	Total dimming

	2
	000-255
	stroboscopic

	three
	000-255
	R red lamp bead linear dimming

	four
	000-255
	G linear dimming of green lamp beads

	five
	000-255
	B linear dimming of blue lamp beads

	six
	000-255
	W white lamp bead linear dimming

	seven
	000-255
	Macro color

	eight
	000-255
	model

	nine
	000-255
	speed

	10
	000-255
	direction

	11
	000-255
	background color

	12
	000-255
	Background tone light


CH144 channel table description:
	passage
	Channel value
	Basic function of channel

	one
	000-255
	Linear dimming of the first red lamp bead

	2
	000-255
	Linear dimming of the first green lamp bead

	three
	000-255
	Linear dimming of the first blue lamp bead

	four
	000-255
	Linear dimming of the first white lamp bead

	…
	…
	… …

	141
	000-255
	Linear dimming of the 36th red lamp bead

	142
	000-255
	Linear dimming of the 36th green lamp bead

	143
	000-255
	Linear dimming of the 36th blue lamp bead

	144
	000-255
	Linear dimming of the 36th white lamp bead





VII. Technical parameters
[bookmark: OLE_LINK5]Voltage: AC100~240V 50/60HZ
Power: 200W
Lamp beads: 36 8W four-in-one LED lamp beads
Control mode: DMX512, self-propelled, master-slave, voice control, RDM.
Channels: select channels CH04, CH12 and CH144.
Dimming: 32bit 0~100% linear dimming	
Features: dyeing+flash
Working temperature: -30 ~50℃
Strobe frequency: 1~30HZ
Appearance: metal, black
Connection mode: DMX512 input/output/power input/output.
IP grade: IP20
Size: weight:
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