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	Lighting Specifications
	Parameters

	[bookmark: _Hlk224838722]Product Name
	Waterproof Moving Head Strobe Light
	Light Color
	Black
	Input Voltage: AC100V-240V 50/60HZ
Power Consumption: 1400W
RGB color washing light source：
784 pcs×1.5W×3-color 5050 LED
White light strobe light source：
392 pcs×2W Cool White LED
RGB Zones：14 independently controllable zones
White Light Zones：28 independently controllable zones
CCT：Approx. 6000K (Daylight)
Beam Angle：Combined light 98°×57°, strobe light 95°× 50°
Luminous Flux：Up to 71620 lumens
Tilt Range：180°electronic tilt
Operating Temperature: -10℃～+40℃
Dimming：16-bit high-precision dimming for ultra-smooth transitions
Strobe：Electronic strobe, rate 0–30 Hz
Other Features：Adjustable PWM frequency (up to 25kHz) for flicker-free filming
Control Mode: DMX、Art-Net、sACN、RDM
[bookmark: _GoBack]Channel：8CH /11CH /13CH /14CH /24CH /30CH /47CH /74CH /97CH 
IP Rating:IP65
Product Dimensions: 406*339.4*202mm
Net Weight: 11.5kg

in-1 strobe & wash effect, 180° electric pan, rich varied effects.

High brightness output, pixel-level precise control, ideal for large stages and outdoor performances.

	Net Weight
	11.5kg
	Gross Weight
	14.5kg
	

	Product Dimensions
	406*339.4*202mm
	Lighting Material
	All-magnesium alloy body 
	

	Optical System/Effect System
	

	RGB color washing light source
	784 pcs×1.5W×3-color 5050 LED
	White light strobe light source
	392 pcs×2W Cool White LED
	

	RGB Zones
	14 independently controllable zones
	White Light Zones
	28 independently controllable zones
	

	Beam Angle
	Combined light 98°×57°, strobe light 95°× 50°
	CCT
	Approx. 6000K (Daylight)
	

	Tilt Range
	180°electronic tilt
	Dimming
	16-bit high-precision dimming for ultra-smooth gradient effect
	

	Luminous Flux
	Up to 71620 lumens
	Strobe
	Electronic strobe, rate 0–30 Hz
	

	Effect Light
	2- in-1 strobe & wash effect, 180° electric pan, rich varied effects.
	Other Features
	Adjustable PWM frequency (up to 25kHz) for flicker-free filming
	

	Electrical Connection
	Control System
	

	Input Voltage
	AC100V-240V 50/60HZ
	Mechanical Movement
	Vertical Scanning Angle 221°, Automatic Return Correction and 16bit Precision Fine-Tuning Function
	

	Total Lamp Power
	1400W
	Communication Design
	DMX Wired/Wireless Transmission, Convenient and Fast Software Upgrade via DMX Data Cable
	

	Signal Connection
	3-pin / 5-pin waterproof signal cable & XLR socket & RJ45 interface
	Heat Dissipation System
	Fan Heat Dissipation Structure and Temperature Intelligent Monitoring Technology, Automatically Adjusts Heat Dissipation System to Effectively Control Lamp Temperature
	

	Power Connection
	Waterproof Power I/O & Xishan Connector I/O
	Control Protocol
	DMX、Art-Net、sACN、RDM
	

	Display Screen
	Fixture and lamp usage time can be queried for easy maintenance
	Channel Mode
	8CH/11CH/13CH/14CH/24CH/30CH/47CH/74CH/97CH 
	

	Photometric Diagram
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