Function description of fireworks machine
	Passageway
	Control function
	Numerical value
	The nixie tube shows


 
	1
	Off
	000~009
	A001 DMX address code

	
	Spray height 1
	010~019
	

	
	Spray height 2
	020~029
	

	
	Spray height 3
	030~039
	

	
	Spray height 4
	040~049
	

	
	Spray height 5
	050~059
	

	
	Spray height 6
	060~069
	

	
	Spray height 7
	070~079
	

	
	Spray height 8
	080~089
	

	
	Spray height 9
	090~099
	

	
	Spray height 10
	100~255
	

	
2
	Heating off
	000~009
	A001 DMX address code

	
	Heat on
	010~239
	Displays the current temperature value

	
	Emergency stop
	240~255
	STOP




2、 Panel description


1. Key description
Key sequence from left to right: Menu-> Up-> Down-> Confirm

1) Menu: switch the menu interface to the next menu.
2) Up: it can be used for menu switching, and the previous menu can be used; when the confirmation key is pressed, it will be added up. In the DMX address code interface, the address code will be added up; in the working temperature setting interface, the working temperature will be increased up.
3) Down: when the confirmation key is pressed down, the address code will be decreased down in the DMX address code interface; the working temperature will be decreased down in the working temperature setting interface.
4) Confirm: The interface enters the setting state, and the current interface can add or subtract values. (Valid only under address code and operating temperature)

2. Indicator light description
1) Yellow light: flashing indicates that the working temperature has not been reached; if it is on, it indicates that the heating is completed and the working temperature has been reached.
2) Green light: If it is on, it indicates that there is DMX signal; if it is off, it indicates that the signal is disconnected.
3) Red light: the light is on when there is an error, for example, there is a problem with the temperature control detection or the heating.
4) Blue light: always on when heating.


3. Interface description (press the menu key or up key to switch the interface)

1） Address code interface:


Operating instructions: press the confirmation key to enter the editing, select the address code 001-512, and then press the confirmation key to exit the address code editing.

2） Temperature interface:


Operating instructions: The current interface cannot be operated, and only the current temperature status can be displayed in real time.





3） Working temperature setting interface:


Operating instructions: Set the working temperature, and spray the flowers when the temperature is heated to the current temperature; press the confirmation key to enter the editing, select the temperature range of 560-620 degrees, and then press the confirmation key to exit the editing state.


4） Error reporting interface:


Operating instructions: The current interface cannot be operated, and only appears when an error is reported.
E01: an error is reported when the temperature is lower than 10 ℃ after heating for 2 minutes;
E02: An error is reported when the temperature does not reach the working temperature in the state of heating for half an hour without spraying;
E03: The temperature is too high and an error is reported;
E04: detect that the temperature control is abnormal and report an error;









5） Wireless Interface:
1. Slave interface

2. Host interface


Operating instructions: press the confirmation key to enter the master-slave switch.





















3、 Remote control instructions


1) Press key A: press it once to heat, observe that the blue indicator light is on and the temperature display interface is adjusted to heat, the heating state is increased, and press key A again to stop heating.
2) Key B: When the heating temperature is reached, press key B to select spray height 1; during spraying, press key B to stop spraying.
3) Key C: When the heating temperature is reached, press key C to select spray height 2; during spraying, press key C to stop spraying.
4) Key D: When the heating temperature is reached, press key D to select spray height 3; during the spray process, press key D to stop spraying.
5）Long Press 6 key for 5 seconds to start the function, then press 6 key once stop
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