1、 4-color DMX channel menu
AH40 DH41
8-channel mode (A001 state)
	passage
	function
	explain

	CH1
	Total dimming
	Total dimming, from dark to bright

	CH2
	R dimming
	Red dimming, from dark to bright.

	CH3
	G dimming
	Green dimming, from dark to bright

	CH4
	B dimming
	Blue dimming, from dark to bright

	CH5
	W dimming
	White dimming, from dark to bright

	CH6
	Total stroboscopic
	Global stroboscopic, from slow to fast

	CH7
	FS
	0: Dimming mode; 1-62: color selection (selected by CH8); 63-124: saltus step; 125-186: gradual change; 187-249:  pulse change; 250-255: Voice control (CH8 selects voice control 1 and 2)

	CH8
	Functional speed
	Function speed, from slow to fast (color selection for color output, sound control strobe and jump for voice control)



8-channel mode (d001)
	passage
	function
	explain

	CH1
	Total dimming
	Total dimming, from dark to bright

	CH2
	Total stroboscopic
	Global stroboscopic, from slow to fast

	CH3
	FS
	0: Dimming mode; 1-62: color selection (selected by CH4); 63-124: Jump; 125-186: gradual change; 187-249 pulse change; 250-255: Voice control (CH4 selects voice control 1 and 2)

	CH4
	Functional speed
	Function speed, from slow to fast (color selection for color output, sound control strobe and jump for voice control)

	CH5
	R dimming
	Red dimming, from dark to bright.

	CH6
	G dimming
	Green dimming, from dark to bright

	CH7
	B dimming
	Blue light, from dark to bright

	CH8
	W dimming
	White dimming, from dark to bright



Second, the digital tube display menu description
	serial number
	content
	scale
	Function and description

	one
	A001
	001- 512
	DMX512 address code setting -8-channel mode

	2
	d001
	001- 512
	DMX512 address code setting -8-channel mode

	three
	r255
	000 - 255
	Red dimming, from dark to bright.

	four
	G255
	000 - 255
	Green dimming, from dark to bright.

	five
	b255
	000 - 255
	Blue dimming, from dark to bright.

	six
	u255
	000 - 255
	White dimming, from dark to bright.

	seven
	FH99
	01 - 99
	Strobe, speed from slow to fast.

	eight
	CL01
	01 - 15
	Manual color selection mode.

	nine
	CC99
	01 - 99
	Jump from slow to fast.

	10
	DE99
	01 - 99
	Gradient, from slow to fast.

	11
	CP99
	01 - 99
	Pulse changes from slow to fast.

	12
	SU01
	01 - 02
	Mode: 1 is stroboscopic jump, 2 is jump.




Third, the master-slave machine description
Automatically receive the slave signal in d001 or A001 state, without setting it separately.


4， Types of applicable lamps and lanterns
1,4-eye COB surface light lamp ()

2, 18 24 4-in-1 color surface lights ()

3,2-eye bicolor COB surface light lamp ()
