
LED operating instructions for stage lighting equipment





                       


(Please read the instructions carefully and carefully before using the product)
For proper and safe use, read the instructions carefully before installing and using the product. This specification contains important installation and application information, please strictly follow the instructions when installing and operating the product. At the same time, please keep this instruction manual properly.
Our 230W beam lamp uses a new and beautiful high-temperature resistant metal body. This product strictly follows the CE standard for design and production, in line with the international standard DMX512 signal protocol, can be used separately for control, can also be used online, with fast rotation, low noise, powerful features, suitable for small and medium-sized concerts, theaters, studios, nightclubs and bars and other places,
Please remove the package carefully, check whether the product is damaged during transportation, and check whether the following contents are complete.
          
Beam lamp- - - - - - - - -1 set             Instruction manual- - - - - - - -1 version
          Power cord- - - - - - - - -1 piece             Signal line- - - - - - - - -1 bar                 
This product is a good product before delivery. In order to keep the product in good condition and ensure safe operation, users should follow the safety matters and the instructions.
Important: Damage caused by not following this instruction is not covered by the warranty. The supplier is not responsible for the product problems arising from this.
If the product has been exposed to extreme unstable temperature (e. g. after transportation), do not power the product immediately because water drops due to temperature changes may damage the product. Please use it after the product has returned to the normal temperature.
This product can be used in the voltage range of 90-240V, and is used for indoor products. Please confirm that the voltage used is not above the tolerable range of the product!! The power plug must be plugged into a protective class I socket. Green or tea-cyan conductors must be grounded.
Please check the product and the power cord frequently. Ensure that the power cord is not folded or damaged and not connected to other wires! Special attention is required when connecting the power cord or the related wiring. Unplug the power supply without using the product or before cleaning.
Before using the product, please be familiar with the operation function of the product. Please do not expose children or no professionals to the product. Please do not shake this product. Do not use brute force when installing or operating the product. Do not allow unprofessionals to operate the product. Most of the damage is caused by an unprofessional operation.
The product is not equipped with relevant repair accessories. The maintenance and repair of the products can only be carried out by professionals!
Please do not change this product without authorization, otherwise the product may be damaged, so the damage caused is not covered by the warranty. Also, unprofessional operations can lead to short circuits, burns or electric shocks, and so on.




DMX512 Connection of the signal:
This lamp uses DMX512 signal control mode, and the control signal of each lamp is in parallel. When connecting the signals of multiple lamps, it is best to use dual-core shielding cable. When connecting, each lamp is connected through the DMX signal jack (Canon seat) INPUT (input) and OUTPUT (output). The 3-core XLR plug terminal of the signal line connecting the lamp must correspond to each other. When connecting the lamp signal, it is recommended to use the DMX signal terminal. It is possible to destroy the control signal due to electrical noise. The DMX signal terminal is a 120 ohm 1W resistance between the 2 and 3 feet of an XLR plug and connects it to the OUTPUT (output) jack of the last lamp.
Calculation method of lamp starting address code:
The starting address code of the current lamp is equal to (the starting address code of the previous lamp) + (number of channels of the lamp) description:
1: Start address code value of the first lamp A001.
2: The basic number of controller should be greater than or equal to the total number of lighting channels.
3: Note: when any controller is used, each lamp must have its own starting address code. If the starting address code of the first lamp is set A001, the pass number of the lamp is 16 CH; then the starting address code of the second lamp is set to A017; the starting address code of the third lamp is set to A033; and so on, (this setting mode should be determined by different console).

Product Parameter:
Input voltage: AC100V-220V 50 / 60Hz
Power: 450W
Color plate: 12 colors + white light
Colorful color: six-color plate
Fixed pattern: 13 patterns + white light
Prism: a single prism
Aization: six color rainbow + atomization integration
Horizontal / vertical: 540° horizontal scan, 270° vertical scan
Display interface: color screen 1.8 inch button, 180° reverse display can be switched in Chinese and English
Protection level: IP20

	Menu Action Settings

	primary menu
	Submenu one
	Function Settings
	Functional profile

	DMX address
	
	1-512
	

	System Settings
	Show upside down
	normal
	.

	
	
	overturn
	

	
	Language setting
	the Chinese language
	

	
	
	English
	

	
	channel pattern
	20CH
	

	
	running mode
	DMX
	

	
	
	sound control
	

	
	
	voluntarily
	

	
	Electronic lighting
	close
	

	
	
	open
	

	
	The bulb default
	Turn on _ Close
	

	
	Bulb control
	illume
	

	
	optimal path
	Turn on _ Close
	

	
	Horizontal reverse
	close
	

	
	
	open
	

	
	Vertical reverse
	close
	

	
	
	open
	

	
	XY velocity
	low speed
	

	
	
	intermediate speed
	

	
	
	fast
	

	
	Optical coupling detection
	close
	

	
	
	open
	

	
	Return to the superior
	▲
	

	information services
	total time
	0-9999
	

	
	Light bulb time
	0-9999
	

	
	binding hours
	0-9999
	

	
	display software
	Vx001
	

	
	XY software
	Vx001
	

	
	Small motor software
	Vx001
	

	
	Return to the superior
	▲
	

	Channel control
	Color hovering
	0-255
	

	
	stroboflash
	0-255
	

	
	aiming"
	0-255
	

	
	Fixed pattern
	0-255
	

	
	prism
	0-255
	

	
	Prism rotation
	0-255
	

	
	atomization
	0-255
	

	
	focus
	0-255
	

	
	Horizontal rotation
	0-255
	

	
	Horizontal fine-tuning
	0-255
	

	
	vertical turn
	0-255
	

	
	Vertical fine-tuning
	0-255
	

	
	reset
	0-255
	

	
	light up
	0-255
	

	
	XY velocity
	0-255
	

	
	Color disk speed
	0-255
	

	
	Zoom speed
	0-255
	

	
	pattern velocity
	0-255
	

	
	Return to the superior
	0-255
	

	operative mode
	XY communication
	normal
	current state

	
	
	wrong
	

	
	Small motor communication
	normal
	

	
	
	wrong
	

	
	Focus hall
	normal
	

	
	
	wrong
	

	
	Color plate hall
	normal
	

	
	
	wrong
	

	
	Pattern hall
	normal
	

	
	
	wrong
	

	
	X optocoupler
	normal
	

	
	
	wrong
	

	
	Y optocoupler
	normal
	

	
	
	wrong
	

	
	Fan speed
	6500
	

	
	Return to the superior
	▲
	

	auxiliary neans
	Calibration code 1
	0-9999
	

	
	total time
	zero clearing
	

	
	
	carry out
	

	
	Light gun time
	zero clearing
	

	
	
	carry out
	

	
	Restore the default
	give tacit consent to
	

	
	
	recover
	

	
	
	preserve
	

	
	Horizontal rotation
	0-255
	Zero-bit initial bits

	
	vertical turn
	0-255
	

	
	focus
	0-255
	

	
	Prism # # 1
	0-255
	

	
	Prism mirror 2
	[bookmark: _GoBack]0-255
	

	
	Prism rotation 1
	0-255
	

	
	Prism rotation 2
	0-255
	

	
	atomization
	0-255
	

	
	Color combination
	0-255
	

	
	Fixed pattern
	0-255
	

	
	colour disk
	0-255
	

	
	stroboflash
	0-255
	

	
	Flash midpoint
	0-255
	

	
	Prism a point
	0-255
	

	
	Prism two points
	0-255
	

	
	Fog midpoint
	0-255
	

	
	Colorful midpoint
	0-255
	

	
	Return to the superior
	▲
	

	advanced setup
	Check code 2
	0-9999
	

	
	Signal encryption
	open
	

	
	
	close
	

	
	DMX velocity
	0-255
	

	
	DMX data packet
	0-255
	

	
	DMX type
	0-055
	

	
	DMX insulate
	0-65535
	A smaller value would indicate a more stable signal

	
	Drive plate temperature
	<110 Degrees>
	Red appears beyond this range

	
	Drive board is 3.3V
	3.0V - 3.6V
	Red appears beyond this range

	
	Drive board: 5.0V
	4.5V - 5.5V
	Red appears beyond this range

	
	Drive board 12V
	10.0V - 14.0V
	Red appears beyond this range

	
	Drive board 36V
	20.0V - 42.0V
	Red appears beyond this range

	
	X state
	static
	

	
	
	turn
	

	
	X Hoare
	normal
	

	
	
	wrong
	Show red

	
	X-light coupling phase
	0-3
	

	
	X optocoupler A
	40-160
	Standard setting 100 shows red beyond the required range, but the panel red light does not alarm

	
	X optocoupler B
	40-160
	Standard setting 100 shows red beyond the required range, but the panel red light does not alarm

	
	X optocoupler C
	40-160
	Standard setting 100 shows red beyond the required range, but the panel red light does not alarm

	
	X optocoupler D
	40-160
	Standard setting 100 shows red beyond the required range, but the panel red light does not alarm

	
	X Current Angle
	000-540
	

	
	X drive state
	normal
	

	
	
	wrong
	Show red

	
	Y state
	static
	

	
	
	turn
	

	
	Y optocoupler
	normal
	

	
	
	wrong
	Show red

	
	Y Hoare
	normal
	

	
	
	wrong
	Show red

	
	Y light coupling phase
	0-3
	

	
	Y optocoupler A
	40-160
	Red appears beyond this range

	
	Y optocoupler B
	40-160
	Red appears beyond this range

	
	Y optocoupler C
	40-160
	Red appears beyond this range

	
	Y optocoupler D
	40-160
	Red appears beyond this range

	
	Y Current Angle
	000-250
	

	
	Y drive state
	normal
	

	
	
	wrong
	Show red

	
	Return to the superior
	▲
	

	Channel level
	Color hovering
	0-255
	Current DMX channel value

	
	stroboflash
	0-255
	

	
	aiming
	0-255
	

	
	Fixed pattern
	0-255
	

	
	prism
	0-255
	

	
	Prism rotation
	0-255
	

	
	atomization
	0-255
	

	
	focus
	0-255
	

	
	Horizontal rotation
	0-255
	

	
	Horizontal fine-tuning
	0-255
	

	
	vertical turn
	0-255
	

	
	Vertical fine-tuning
	0-255
	

	
	reset
	0-255
	

	
	light up
	0-288
	

	
	XY velocity
	0-255
	

	
	Color disk speed
	0-255
	

	
	Zoom speed
	0-255
	

	
	pattern velocity
	0-255
	

	
	Return to the superior
	
	

	reset
	Full reset
	cancel
	manual reset

	
	
	carry out
	

	
	XY reset
	cancel
	

	
	
	carry out
	

	
	Effect reset"
	cancel
	

	
	
	carry out
	

	
	Return to the superior
	
	

	Exit menu
	
	
	

	16 Channel table

	CH1
	pigment
	0--4
	white light

	
	
	5--9
	White light + color 1

	
	
	10--14
	Color 1

	
	
	15--19
	Color # 1 + color # 2

	
	
	20--24
	Color 2

	
	
	25--29
	Color # 2 + color # # 3

	
	
	30--34
	Color 3

	
	
	35--39
	Color # 3 + color # # 4

	
	
	40--44
	Color 4

	
	
	45-49
	Color # 4 + color # # 5

	
	
	50--54
	Color 5

	
	
	55--59
	Color # 5 + color # # 6

	
	
	60--64
	Color 6

	
	
	65--69
	Color # 6 + color # # 7

	
	
	70--74
	Color 7

	
	
	75--79
	Color # 7 + color # # 8

	
	
	80--84
	Color 8

	
	
	85--89
	Color # 8 + color # # 9

	
	
	90--94
	Color 9

	
	
	95--99
	Colour 9 + color 10

	
	
	100--104
	Color 10

	
	
	105--109
	Colour 10 + color 11

	
	
	110--114
	Color 11

	
	
	115--119
	Colour 11 + color 12

	
	
	120--124
	Color 12

	
	
	125--129
	Colour 12 + color 13

	
	
	130--135
	white light

	
	
	136--195
	From fast to slow forward flowing water

	
	
	196--255
	From fast to slow reverse flow water

	CH2
	stroboflash
	0-5
	The light switch is closed

	
	
	6--20
	Open the flash

	
	
	21-70
	Synchronize the strobe slow to fast

	
	
	71-100
	Random strobe is slow to fast

	
	
	101-150
	Pulse strobe is slow to fast

	
	
	151-190
	The open pulse is slow to fast

	
	
	191-230
	Turn-off pulse frequency strobe is slow to fast

	
	
	231-255
	The light switch is opened

	CH3
	aiming
	0-255
	With 0-100% dimming

	CH4
	pattern
	0--4
	White aperture

	
	
	5--9
	Pattern 1

	
	
	10--14
	Pattern 2

	
	
	15--19
	Pattern 3

	
	
	20--24
	Pattern 4

	
	
	25--29
	Pattern 5

	
	
	30--34
	Pattern 6

	
	
	35--39
	Pattern 7

	
	
	40--44
	Pattern 8

	
	
	45-49
	Pattern 9

	
	
	50--54
	Pattern 10

	
	
	55--59
	Pattern 11

	
	
	60--64
	Pattern 12

	
	
	65--69
	Pattern 13

	
	
	70-125
	From fast to slow counterclockwise flow water

	
	
	126-130
	Stop running water

	
	
	131-190
	From slow to fast counterclockwise flow water

	
	
	191-195
	Pattern 1 shakes from slow to fast

	
	
	196-200
	Pattern 2 shakes from slow to fast

	
	
	201-205
	Pattern 3 shakes from slow to fast

	
	
	206-210
	Pattern 4 shakes from slow to fast

	
	
	211-215
	Pattern 5 shakes from slow to fast

	
	
	216-220
	Pattern 6 shakes from slow to fast

	
	
	221-225
	Pattern 7 shakes from slow to fast

	
	
	226-230
	Pattern 8 shakes from slow to fast

	
	
	231-235
	Pattern 9 shakes from slow to fast

	
	
	236-240
	Pattern 10 shakes from slow to fast

	
	
	241-245
	Pattern 11 shakes from slow to fast

	
	
	246-250
	Pattern 12 from slow to fast

	
	
	251-255
	Pattern 13 with a jitter ranging from slow to fast

	CH5
	prism
	0-127
	Remove the prism

	
	
	128-255
	Prism cut in

	CH6
	Prism rotation
	0-127
	0-400 degrees

	
	
	128-189
	From fast to slow reverse flow water

	
	
	190-194
	cease

	
	
	195-255
	From slow to fast forward flowing water

	CH7
	Reserved empty
	
	

	CH8
	Fog colorful
	0-127
	

	
	
	128-169
	Insert atomization

	
	
	170-255
	Insert colorful

	CH9
	focus
	0-255
	From far to near

	CH10
	X axle
	0-255
	0-540 degrees

	CH11
	X axis fine-tuning
	0-255
	The X-axis 16bit fine-tuning channel

	CH12
	Y axle
	0-255
	0-240 degrees

	CH13
	Y axis fine-tuning
	0-255
	Y axis 16bit tuning channel

	CH14
	XY velocity
	0-255
	

	CH15
	Reserved empty
	0-255
	NC

	CH16
	Light reset
	0-99
	NF

	
	
	100-105
	Off-bulb (5S)

	
	
	106-199
	NF

	
	
	200-205
	Open the light bulb (5S)

	
	
	206-249
	NF

	
	
	250-255
	All motor reset (5S)



Instructions for lamp installation:
This lamp can be placed horizontally, oblique hanging and upside down, oblique hanging and upside down must pay attention to the installation method. Fixed installation of lamps: before the positioning of lamps, ensure the stability of the installation site, the lamps must not fall off the support frame, and use the support frame and the safety rope for auxiliary hanging; to ensure safety. Prevent the falling and sliding of the lamps and lanterns. During the installation and debugging, the safety rope is worn and the hook screw is loose. If the hanging installation is not stable, and all the consequences of the falling, the manufacturer will not bear any responsibility.


after-sale service
pay attention to! When the lamps leave the factory, they are passed by strict quality inspection, and the packaging is in good condition. Please operate according to the instructions. Machine failure caused by human causes is not covered by the warranty.
1. The company provides technical advice to our clients for life.
2. If the product is faulty and needs to be repaired, please show the product warranty card and fill in the relevant content truthfully. At the same time, we also hope that customers can feedback the problems of the product to us in time, so as to facilitate us to improve the product in the first time









