	7 Bee Eye Menu Operation Settings

	primary menu
	Submenu 1
	Function setting
	Brief introduction of function

	DMX address
	
	1-512
	

	system setup
	Display backward
	normal
	.

	
	
	turn
	

	
	Language settings
	Chinese
	

	
	
	English
	

	
	Channel mode
	20CH
	

	
	operational mode
	DMX
	

	
	
	sound-controlled
	

	
	
	automatic
	

	
	Master-slave mode
	From the machine
	

	
	
	host machine
	

	
	Dimming mode
	ON_ OFF
	

	
	Horizontal reversal
	close
	

	
	
	open
	

	
	Vertical inversion
	close
	

	
	
	open
	

	
	XY speed
	low speed
	

	
	
	intermediate speed
	

	
	
	fast
	

	
	Optocoupler detection
	close
	

	
	
	Open open
	

	
	Signal clearing
	Turn Off
	

	
	
	Open open
	

	
	Sensitive voice control
	0-100%
	

	
	Bai Pingheng
	Turn Off
	

	
	
	Open open
	

	
	White balance red
	0-255
	

	
	White balanced green
	0-255
	

	
	White balance blue
	0-255
	

	
	White balance white
	0-255
	

	
	Return to the superior
	▲
	

	Channel control
	Red color
	0-255
	

	
	Red fine tuning
	0-255
	

	
	Green color
	0-255
	

	
	Green fine tuning
	0-255
	

	
	Blue color
	0-255
	

	
	Blue fine tuning
	0-255
	

	
	White color
	0-255
	

	
	White fine tuning
	0-255
	

	
	Color temperature
	0-255
	

	
	Yansehong
	0-255
	

	
	Frequency flash
	0-255
	

	
	aiming
	0-255
	

	
	Dimming and fine tuning
	0-255
	

	
	Horizontal rotation
	0-255
	

	
	Horizontal fine adjustment
	0-255
	

	
	Vertical rotation
	0-255
	

	
	Vertical fine tuning
	0-255
	

	
	Function setting
	0-255
	

	
	Complex position
	0-255
	

	
	Focus adjustment
	0-255
	

	
	Focusing rotation
	0-255
	

	
	LED effect
	0-255
	

	
	LED speed
	0-255
	

	
	Effect gradient
	0-255
	

	
	Effect red
	0-255
	

	
	Effect green
	0-255
	

	
	Effect blue
	0-255
	

	
	Effect white
	0-255
	

	
	Effect dimming
	0-255
	

	
	Background dimming
	0-255
	

	
	Excessive effect
	0-255
	

	
	Effect angle
	0-255
	

	
	Foreground stroboscopic
	0-255
	

	
	Background stroboscopic
	0-255
	

	
	Background selection
	0-255
	

	
	Return to the superior
	0-255
	

	functional mode
	Total time
	0-9999
	current state

	
	Motherboard software
	Vxxx
	

	
	Focusing hall
	normal
	

	
	
	mistake
	

	
	Rotating hall
	normal
	

	
	
	mistake
	

	
	X-optical coupler
	normal
	

	
	
	mistake
	

	
	Y optocoupler
	normal
	

	
	
	mistake
	

	
	Temperature detection
	0-120
	

	
	Return to the superior
	▲
	

	appurtenance
	Check code 1
	0-9999
	

	
	Check code 1
	▲
	

	
	Total time
	clear
	

	
	
	carry out
	

	
	Restore default
	default
	

	
	
	recover
	

	
	
	preserve
	

	
	Lamp bead 1 red
	0-255
	

	
	Lamp bead 1 green
	0-255
	

	
	Lamp bead 1 blue
	0-255
	

	
	Lamp bead 1 white
	0-255
	

	
	Lamp bead 2 red
	0-255
	

	
	Lamp bead 2 green
	0-255
	

	
	Lamp bead 2 blue
	0-255
	

	
	Lamp bead 2 white
	0-255
	

	
	Lamp bead 3 red
	0-255
	

	
	Lamp bead 3 green
	0-255
	

	
	Lamp bead 3 blue
	0-255
	

	
	Lamp bead 3 white
	0-255
	

	
	Lamp bead 4 red
	0-255
	

	
	Lamp bead 4 green
	0-255
	

	
	Lamp bead 4 blue
	0-255
	

	
	Lamp bead 4 white
	0-255
	

	
	Lamp bead 5 red
	0-255
	

	
	Lamp bead 5 green
	0-255
	

	
	Lamp bead 5 blue
	0-255
	

	
	Lamp bead 5 white
	0-255
	

	
	Lamp bead 6 red
	0-255
	

	
	Lamp bead 6 green
	0-255
	

	
	Lamp bead 6 blue
	0-255
	

	
	Lamp bead 6 white
	0-255
	

	
	Lamp bead 7 red
	0-255
	

	
	Lamp bead 7 green
	0-255
	

	
	Lamp bead 7 blue
	0-255
	

	
	Lamp bead 7 white
	0-255
	

	
	Horizontal rotation
	0-255
	

	
	Vertical rotation
	0-255
	

	
	Focus adjustment
	0-255
	

	
	Focusing rotation
	0-255
	

	
	Return to the superior
	▲
	

	Channel level
	Red color
	0-255
	Only channel values can be queried.

	
	Red fine tuning
	0-255
	

	
	Green color
	0-255
	

	
	Green fine tuning
	0-255
	

	
	Blue color
	0-255
	

	
	Blue fine tuning
	0-255
	

	
	White color
	0-255
	

	
	White fine tuning
	0-255
	

	
	Color temperature
	0-255
	

	
	Yansehong
	0-255
	

	
	Frequency flash
	0-255
	

	
	aiming
	0-255
	

	
	Dimming and fine tuning
	0-255
	

	
	Horizontal rotation
	0-255
	

	
	Horizontal fine adjustment
	0-255
	

	
	Vertical rotation
	0-255
	

	
	Vertical fine tuning
	0-255
	

	
	Function setting
	0-255
	

	
	Complex position
	0-255
	

	
	Focus adjustment
	0-255
	

	
	Focusing rotation
	0-255
	

	
	LED effect
	0-255
	

	
	LED speed
	0-255
	

	
	Effect gradient
	0-255
	

	
	Effect red
	0-255
	

	
	Effect green
	0-255
	

	
	Effect blue
	0-255
	

	
	Effect white
	0-255
	

	
	Effect dimming
	0-255
	

	
	Background dimming
	0-255
	

	
	Excessive effect
	0-255
	

	
	Effect angle
	0-255
	

	
	Foreground stroboscopic
	0-255
	

	
	Background stroboscopic
	0-255
	

	
	Background selection
	0-255
	

	
	Return to the superior
	0-255
	

	Reset all
	cancel
	
	

	
	carry out
	
	

	
	
	
	

	
	
	
	

	Advanced settings
	Signal encryption
	open
	

	
	
	close
	

	
	DMX speed
	0-255
	

	
	DMX data packet
	0-255
	

	
	DMX type
	0-055
	

	
	DMX isolation
	0-65535
	The smaller the value, the more stable the signal is.

	
	LED temperature
	< 110 degrees >
	If it exceeds this range, red will be displayed.

	
	ADC detection
	0-4096
	

	
	X state
	be motionless
	

	
	
	turn
	

	
	X hall
	normal
	

	
	
	mistake
	Show red

	
	X-ray optical coupler phase
	0-3
	

	
	X optocoupler a
	40-160
	The standard setting of 100 exceeds the required range and displays red, but the red light on the panel does not give an alarm.

	
	X optocoupler b
	40-160
	The standard setting of 100 exceeds the required range and displays red, but the red light on the panel does not give an alarm.

	
	X optocoupler c
	40-160
	The standard setting of 100 exceeds the required range and displays red, but the red light on the panel does not give an alarm.

	
	X optocoupler d
	40-160
	The standard setting of 100 exceeds the required range and displays red, but the red light on the panel does not give an alarm.

	
	X current angle
	000-540
	

	
	X drive state
	normal
	

	
	
	mistake
	Show red

	
	Y state
	be motionless
	

	
	
	turn
	

	
	Y optocoupler
	normal
	

	
	
	mistake
	Show red

	
	Y hall
	normal
	

	
	
	mistake
	Show red

	
	Y-coupler phase
	0-3
	

	
	Y optocoupler a
	40-160
	If it exceeds this range, red will be displayed.

	
	Y optocoupler b
	40-160
	If it exceeds this range, red will be displayed.

	
	Y optocoupler c
	40-160
	If it exceeds this range, red will be displayed.

	
	Y optocoupler d
	40-160
	If it exceeds this range, red will be displayed.

	
	Y current angle
	000-250
	

	
	Y drive state
	normal
	

	
	
	mistake
	Show red

	
	Green-blue exchange
	close
	

	
	
	open
	

	
	Return to the superior
	▲
	



Master-slave control
There are two or more identical lamps connected by DMX three-core signal lines, all lamps are modified to any address code of 001~512, and any one is set as the master, while other lamps are slaves, and all slave displays do not flicker; When the master adjusts the effects of gradual change, pulse change, jump, voice control and self-walking, all slaves synchronize the effects of gradual change, pulse change, jump, voice control and self-walking.
Special attention: 1. Only one host can be set for a group of lamps. If there are multiple hosts, all lamps will flash without synchronization.
2. All lamps and lanterns must be used when the DMX512 console is closed.
DMX512 control
Address codes of all lamps and lanterns are set, and all lamps and lanterns are connected to the DMX512 console in parallel with DMX three-core signal lines. The address code stops flashing, indicating that the DMX512 console signal has been sent to the lamps and lanterns. According to the channel description, the DMX512 console is used to control related functions.

	24-channel mode
	

	Channel value
	function
	DMX value
	explain
	

	1
	X axis control
	0 - 255
	X axis control
	

	2
	X-axis fine tuning
	0 - 255
	X-axis fine tuning
	

	3
	Y axis control
	0 - 255
	Y axis control
	

	4
	Y axis fine tuning
	0 - 255
	Y axis fine tuning
	

	5
	XY axis velocity
	0 - 255
	Speed from slow to fast
	

	6
	focus
	0-15
	Focus control dyeing mode Focus cannot be rotated.
	

	
	
	16- 255
	Focus control Bee-eye mode Focus can rotate.
	

	7
	rotate
	0 - 127
	0 to 60 degrees
	

	
	
	128 - 190
	Rotate counterclockwise from slow to fast
	

	
	
	191 - 192
	stop
	

	
	
	193 - 255
	Rotate clockwise from slow to fast
	

	8
	Light strip control
	000-004
	The lamp band goes out
	

	
	
	005-013
	red
	

	
	
	014-022
	green
	

	
	
	023-031
	blue
	

	
	
	032-040
	white
	

	
	
	041-255
	Macro change of light strip color
One color stops at the fastest speed every 3 DMX values.
	

	9
	Total dimming
	0 - 255
	0-100% linear hidden weapons modulation
	

	10
	stroboscopic
	0 - 3
	Lights go out
	

	
	
	4 - 103
	Use the same steps from fast to slow.
	

	
	
	104 - 107
	Light up
	

	
	
	108 - 207
	Pulse strongpoint from fast to slow.
	

	
	
	208 - 212
	Light up
	

	
	
	213 - 225
	High speed random strobe
	

	
	
	226 - 238
	Medium speed random strobe
	

	
	
	239 - 251
	Low speed random strobe
	

	
	
	252 - 255
	Light up
	

	11
	red
	0 - 255
	Red 0-100% brightness adjustment, from dark to bright.
	

	12
	green
	0 - 255
	Green 0-100% brightness adjustment, from dark to bright.
	

	13
	blue
	0 - 255
	Blue 0-100% brightness adjustment, from dark to bright.
	

	14
	white
	0 - 255
	White 0-100% brightness adjustment, from dark to bright.
	

	15
	colour temperature
	0 - 255
	Linear color temperature control high-> low
	

	16
	Color macro
	0 - 4
	without
	

	
	
	5 - 255
	The color macro changes one color every 3 DMX values.
	

	17
	Static effect
	0 - 4
	without
	

	
	
	5 - 204
	A static effect for every 5 DMX values.
	

	
	
	205 - 215
	Static effects switch effects forward in turn.
	

	
	
	216 - 228
	Static effects stop switching.
	

	
	
	229 - 239
	Static effects switch effects forward in turn.
	

	
	
	240 - 245
	The static effect switches quickly at random.
	

	
	
	246 - 250
	Static effect random switching
	

	
	
	251 - 255
	Static effect random switching is slow.
	

	18
	Dynamic effect
Channel control of foreground colors 20,21,22,23
Backcolor 11,12,13,14 channel control
	0 - 4
	without
	

	
	
	5 - 255
	One dynamic effect for every 4 DMX values.
	

	19
	Dynamic effect speed
	0 - 127
	Forward rotation is slow to fast
	

	
	
	128 - 255
	Reverse rotation is fast to slow.
	

	20
	Background color red
	0 - 255
	1-100% background red brightness adjustment, from dark to bright.
	

	21
	Background color green
	0 - 255
	1-100% background blue brightness adjustment, from dark to bright.
	

	22
	Background color blue
	0 - 255
	1-100% background green brightness adjustment, from dark to bright.
	

	23
	Background color is white.
	0 - 255
	1-100% background blue brightness adjustment, from dark to bright.
	

	24
	reset
	0 - 250
	No function
	

	
	
	251 - 255
	The reset time is 5 seconds.
	

	35-channel mode

	Channel value
	function
	DMX value
	explain

	1
	red
	0 - 255
	Red 0-100% brightness adjustment, from dark to bright.

	2
	Red fine tuning
	0 - 255
	Red fine tuning

	3
	green
	0 - 255
	Green 0-100% brightness adjustment, from dark to bright.

	4
	Green fine tuning
	0 - 255
	Green fine tuning

	5
	blue
	0 - 255
	Blue 0-100% brightness adjustment, from dark to bright.

	6
	Blue fine tuning
	0 - 255
	Blue fine tuning

	7
	white
	0 - 255
	White 0-100% brightness adjustment, from dark to bright.

	8
	White fine tuning
	0 - 255
	White fine tuning

	9
	colour temperature
	0 - 255
	Linear color temperature control high-> low

	10
	Color macro
	0 - 4
	without

	
	
	5 - 255
	The color macro changes one color every 3 DMX values.

	11
	stroboscopic
	0 - 3
	Lights go out

	
	
	4 - 103
	Use the same steps from fast to slow.

	
	
	104 - 107
	Light up

	
	
	108 - 207
	Pulse strongpoint from fast to slow.

	
	
	208 - 212
	Light up

	
	
	213 - 225
	High speed random strobe

	
	
	226 - 238
	Medium speed random strobe

	
	
	239 - 251
	Low speed random strobe

	
	
	252 - 255
	Light up

	12
	Total dimming
	0 - 255
	0-100 Linear brightness adjustment

	13
	Total dimming and fine tuning
	0 - 255
	Fine adjustment of dimmer

	14
	X axis control
	0 - 255
	X axis control

	15
	X-axis fine tuning
	0 - 255
	X-axis fine tuning

	16
	Y axis control
	0 - 255
	Y axis control

	17
	Y axis fine tuning
	0 - 255
	Y axis fine tuning

	18
	Light strip control
	000-004
	The lamp band goes out

	
	
	005-013
	red

	
	
	014-022
	green

	
	
	023-031
	blue

	
	
	032-040
	white

	
	
	041-255
	Macro change of light strip color
One color stops at the fastest speed every 3 DMX values.

	19
	reset
	0 - 250
	No function

	
	
	251 - 255
	The reset time is 5 seconds.

	20
	focus
	0-15
	Focus control dyeing mode Focus cannot be rotated.

	
	
	16- 255
	Focus control Bee-eye mode Focus can rotate.

	21
	rotate
	0 - 127
	0 to 60 degrees

	
	
	128 - 190
	Rotate counterclockwise from slow to fast

	
	
	191 - 192
	stop

	
	
	193 - 255
	Rotate clockwise from slow to fast

	22
	Dynamic effect
	0 - 4
	without

	
	
	5 - 255
	One dynamic effect for every 4 DMX values.
Foreground Color 20-23 Channel Control
Backcolor 11-14 Channel Control

	23
	Dynamic effect speed
The foreground color is controlled by channels 24, 25, 26, 27, 28, 29 and 33.
The background color is controlled by channels 1, 2, 3, 4, 5, 6, 7, 8, 9, 30 and 34.
	0 - 127
	Forward rotation is slow to fast

	
	
	128 - 255
	Reverse rotation is fast to slow.

	24
	Dynamic effect fade-in and fade-out time
	0 - 127
	Forward rotation is slow to fast

	
	
	5 - 255
	Reverse rotation is fast to slow.

	25
	Background color red
	0 - 255
	Red shape

	26
	Background color green
	0 - 255
	Green shape

	27
	Background color blue
	0 - 255
	Blue shape

	28
	Background color is white.
	0 - 255
	White shape

	29
	Foreground brightness adjustment
	0 - 255
	Foreground dimmer 0-100%

	30
	Background brightness adjustment
	0 - 255
	Background dimmer 0-100%

	31
	NC
	0 - 255
	NC

	32
	Dynamic effect frame selection
	0 - 255
	Frame selection

	33
	Foreground flashes frequently.
	0 - 4
	No stroboscopic constant light

	
	
	5 - 250
	Strobe fast to slow

	
	
	251 - 255
	No stroboscopic constant light

	34
	Background color stroboscopic
	0 - 4
	No stroboscopic constant light

	
	
	5 - 250
	Strobe fast to slow

	
	
	251 - 255
	No stroboscopic constant light

	35
	Background color macro
	0 - 4
	without

	
	
	5 - 255
	The color macro changes one color every 3 DMX values.

	
	
	
	

	52-channel mode
	

	Channel value
	function
	DMX value
	explain
	

	1
	X axis control
	0 - 255
	X axis control
	

	2
	X-axis fine tuning
	0 - 255
	X-axis fine tuning
	

	3
	Y axis control
	0 - 255
	Y axis control
	

	4
	Y axis fine tuning
	0 - 255
	Y axis fine tuning
	

	5
	XY axis velocity
	0 - 255
	Speed from slow to fast
	

	6
	focus
	0-15
	Focus control dyeing mode Focus cannot be rotated.
	

	
	
	16- 255
	Focus control Bee-eye mode Focus can rotate.
	

	7
	rotate
	0 - 127
	0 to 60 degrees
	

	
	
	128 - 190
	Rotate counterclockwise from slow to fast
	

	
	
	191 - 192
	stop
	

	
	
	193 - 255
	Rotate clockwise from slow to fast
	

	8
	Light strip control
	000-004
	The lamp band goes out
	

	
	
	005-013
	red
	

	
	
	014-022
	green
	

	
	
	023-031
	blue
	

	
	
	032-040
	white
	

	
	
	041-255
	Macro change of light strip color
One color stops at the fastest speed every 3 DMX values.
	

	9
	Total dimming
	0 - 255
	0-100% linear hidden weapons modulation
	

	10
	stroboscopic
	0 - 3
	Lights go out
	

	
	
	4 - 103
	Use the same steps from fast to slow.
	

	
	
	104 - 107
	Light up
	

	
	
	108 - 207
	Pulse strongpoint from fast to slow.
	

	
	
	208 - 212
	Light up
	

	
	
	213 - 225
	High speed random strobe
	

	
	
	226 - 238
	Medium speed random strobe
	

	
	
	239 - 251
	Low speed random strobe
	

	
	
	252 - 255
	Light up
	

	11
	red
	0 - 255
	Red 0-100% brightness adjustment, from dark to bright.
	

	12
	green
	0 - 255
	Green 0-100% brightness adjustment, from dark to bright.
	

	13
	blue
	0 - 255
	Blue 0-100% brightness adjustment, from dark to bright.
	

	14
	white
	0 - 255
	White 0-100% brightness adjustment, from dark to bright.
	

	15
	colour temperature
	0 - 255
	Linear color temperature control high-> low
	

	16
	Color macro
	0 - 4
	without
	

	
	
	5 - 255
	The color macro changes one color every 3 DMX values.
	

	17
	Static effect
	0 - 4
	without
	

	
	
	5 - 204
	A static effect for every 5 DMX values.
	

	
	
	205 - 215
	Static effects switch effects forward in turn.
	

	
	
	216 - 228
	Static effects stop switching.
	

	
	
	229 - 239
	Static effects switch effects forward in turn.
	

	
	
	240 - 245
	The static effect switches quickly at random.
	

	
	
	246 - 250
	Static effect random switching
	

	
	
	251 - 255
	Static effect random switching is slow.
	

	18
	Dynamic effect
Channel control of foreground colors 20,21,22,23
Backcolor 11,12,13,14 channel control
	0 - 4
	without
	

	
	
	5 - 255
	One dynamic effect for every 4 DMX values.
	

	19
	Dynamic effect speed
	0 - 127
	Forward rotation is slow to fast
	

	
	
	128 - 255
	Reverse rotation is fast to slow.
	

	20
	Background color red
	0 - 255
	1-100% background red brightness adjustment, from dark to bright.
	

	21
	Background color green
	0 - 255
	1-100% background blue brightness adjustment, from dark to bright.
	

	22
	Background color blue
	0 - 255
	1-100% background green brightness adjustment, from dark to bright.
	

	23
	Background color is white.
	0 - 255
	1-100% background blue brightness adjustment, from dark to bright.
	

	24
	reset
	0 - 250
	No function
	

	
	
	251 - 255
	The reset time is 5 seconds.
	

	25
	Lamp bead 1 red
	0 - 255
	The brightness is dark to bright.
	

	26
	Lamp bead 1 green
	0 - 255
	The brightness is dark to bright.
	

	27
	Lamp bead 1 blue
	0 - 255
	The brightness is dark to bright.
	

	28
	Lamp bead 1 white
	0 - 255
	The brightness is dark to bright.
	

	29
	Lamp Bead 2 Red
	0 - 255
	The brightness is dark to bright.
	

	30
	Lamp bead 2 green
	0 - 255
	The brightness is dark to bright.
	

	31
	Lamp bead 2 blue
	0 - 255
	The brightness is dark to bright.
	

	32
	Lamp bead 2 white
	0 - 255
	The brightness is dark to bright.
	

	33
	Lamp bead 3 red
	0 - 255
	The brightness is dark to bright.
	

	34
	Lamp bead 3 green
	0 - 255
	The brightness is dark to bright.
	

	35
	Lamp bead 3 blue
	0 - 255
	The brightness is dark to bright.
	

	36
	Lamp bead 3 white
	0 - 255
	The brightness is dark to bright.
	

	37
	Lamp bead 4 red
	0 - 255
	The brightness is dark to bright.
	

	38
	Lamp bead 4 green
	0 - 255
	The brightness is dark to bright.
	

	39
	Lamp bead 4 blue
	0 - 255
	The brightness is dark to bright.
	

	40
	Lamp bead 4 white
	0 - 255
	The brightness is dark to bright.
	

	41
	Lamp bead 5 red
	0 - 255
	The brightness is dark to bright.
	

	42
	Lamp bead 5 green
	0 - 255
	The brightness is dark to bright.
	

	43
	Lamp bead 5 blue
	0 - 255
	The brightness is dark to bright.
	

	44
	Lamp bead 5 white
	0 - 255
	The brightness is dark to bright.
	

	45
	Lamp bead 6 red
	0 - 255
	The brightness is dark to bright.
	

	46
	Lamp bead 6 green
	0 - 255
	The brightness is dark to bright.
	

	47
	Lamp bead 6 blue
	0 - 255
	The brightness is dark to bright.
	

	48
	Lamp bead 6 white
	0 - 255
	The brightness is dark to bright.
	

	49
	Lamp bead 7 red
	0 - 255
	The brightness is dark to bright.
	

	50
	Lamp bead 7 green
	0 - 255
	The brightness is dark to bright.
	

	51
	Lamp bead 7 blue
	0 - 255
	The brightness is dark to bright.
	

	52
	Lamp bead 7 white
	0 - 255
	The brightness is dark to bright.
	



[bookmark: OLE_LINK5]Voltage: AC100~240V 50/60HZ
[bookmark: _GoBack]Power: 150W
Lamp beads: 7 4-in-1 LED lamp beads
Control mode: DMX512, self-propelled, master-slave and voice control,
Channels: CH24, CH35 and CH52
Dimming: 32bit 0~100% linear dimming
Features: shake your head+dye+flash.
Working temperature: -30 ~50℃
Strobe frequency: 1~30HZ
Appearance: metal, black
Connection mode: DMX512 input/output/power input/output.
IP grade: IP20
Size: 27*18*40cm
Weight: 6.15kg
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