460-A385-A114三路奔驰内外大复古灯说明书
I. Definition of Display Panel and Keys
[image: ]
Menu up and down confirmation
Menu key: select function
Up arrow: parameter increment
Down arrow: decreasing parameter
Confirm key: OK and save.

Second, the menu function
Press the menu key after powering on and turning on, and the menu menu will appear in turn; Press the up or down key to modify the function parameters, and press the Enter key to save the current function and parameters (with power-off memory after saving).
Menu menu:
	A001
	
	A512
	Set the address code, modify the address code (A001~A512) up or down, and confirm to save.

	CH06
	
	CH363
	Switch channels CH06, CH08, CH12, CH21, CH22 and CH363 up or down, and confirm the key to save. Default CH12

	N127
	
	N127
	Auxiliary light effect mode, confirm key to save.

	S255
	
	S000
	Modify the running speed of auxiliary light effect up or down (S000~ S255), and confirm to save.

	E000
	
	E017
	In the middle main light mode, confirm the key to save.

	S255
	
	S000
	Modify the running speed of the intermediate main light up or down (S000~ S255), and confirm to save.

	Soud
	
	Soud
	Voice control mode.

	U255
	
	U000
	Article 1: White light brightness, modify the brightness of monochromatic light (U000~U255) up or down, and press the Enter key to save.

	V255
	
	V000
	Article 2 White light brightness: modify the brightness of monochromatic light (V000~V255) up or down, and press the Enter key to save.

	W255
	
	W000
	Article 3 White light brightness: modify the brightness of monochromatic lights (W000~W255) up or down, and press the Enter key to save.

	R255
	
	R000
	The internal auxiliary light is dimmed by the red light bulb. Modify the brightness of the red light bulb (R000~ R255) up or down, and press the Enter key to save.

	G255
	
	G000
	The interior auxiliary light is dimmed by the green light bulb, and the brightness of the green light bulb (G000~ G255) is modified up or down, and the Enter key is used to save.

	B255
	
	B000
	The internal auxiliary light is dimmed by the blue light bulb, and the brightness of the blue light bulb is modified up or down (B000~ B255), and the Enter key is used to save.

	X255
	
	X000
	The external auxiliary light is dimmed by the red light bulb, and the brightness of the red light bulb is modified up or down (X000~ X255). Press the Enter key to save.

	Y255
	
	Y000
	The external auxiliary light is dimmed by the green light bulb, and the brightness of the green light bulb (Y000~ Y255) is modified up or down, and the Enter key is used to save.

	Z255
	
	Z000
	The external auxiliary light is dimmed by the blue light bulb, and the brightness of the blue light bulb (Z000~ Z255) is modified up or down, and the Enter key is used to save.

	T000
	
	
	Display the temperature, such as T045, indicating that the current lamp temperature is 45℃.



Third, master-slave control
Two or more identical lamps are connected by DMX three-core signal lines, all lamps are set to any address code A001~A512, and any one is set as the master, while other lamps are slaves, and all slave displays do not flicker; When the master adjusts the effects of gradual change, pulse change, jump, voice control and self-walking, all slaves synchronize the effects of gradual change, pulse change, jump, voice control and self-walking.
Special attention: 1. Only one host can be set for a group of lamps. If there are multiple hosts, all lamps will flash without synchronization.
2. All lamps and lanterns must be used when the DMX512 console is closed.


Fourth, the factory settings
Press the menu key for 3 seconds to enter the factory setting when any address code is A001~A512. Factory settings mainly include the functions of each output power of lamps and lanterns, fan setting mode, setting temperature protection point and sending parameters. The factory sets any mode and presses the menu button for 3 seconds to exit.
Factory Settings Table:
	R255
	
	R020
	R red light bulb current setting, modify the hexagonal red light bulb current (R020-R255) up or down, and confirm to save.

	G255
	
	G020
	G green light bulb current setting, modify the hexagonal green light bulb current (G020-G255) up or down, and confirm to save.

	B255
	
	B020
	B blue light bulb current setting, modify the hexagonal blue light bulb current up or down (B020-B255), and confirm to save.

	W255
	
	W020
	W monochrome lamp current setting, modify the monochrome lamp current setting up or down (W020~W255), and press the Enter key to save.

	FAN1
	
	FAN0
	Fan setting: start the fan as soon as the FAN0 light bulb lights up, and start the fan as soon as the FAN1 reaches the set temperature protection point, and press the Enter key to save.

	T040
	
	T-105
	Set the temperature protection point, modify the parameters (40℃~75℃) up or down, and press the Enter key to save.

	Send
	
	Send
	Send the factory setting parameters of this machine up or down to all other lamps with three-core signal lines connected in parallel; Confirm the sending parameters and press the menu button for 3 seconds.
Exit, deny the parameter and press the confirm key to cancel sending.



V. DMX512 console
After electrifying, the address codes of all lamps and lanterns are set, and all lamps and lanterns are connected to the DMX512 console in parallel with three-core signal lines, and the address codes will stop flashing, indicating that the DMX512 console signal has been sent to the lamps and lanterns. According to each channel description, the DMX512 console is used to control related functions.
CH06 channel description:
	passage
	Channel value
	fundamental function

	passage
	Channel value
	fundamental function

	one
	000-255
	Baiyi

	2
	000-255
	White 2

	three
	000-255
	White 3

	four
	000-255
	R

	five
	000-255
	G

	six
	000-255
	B




CH08 channel description:
	passage
	Channel value
	fundamental function

	passage
	Channel value
	fundamental function

	one
	000-255
	Baiyi

	2
	000-255
	White 2

	three
	000-255
	White 3

	four
	000-255
	Internal mode

	five
	000-255
	Internal velocity

	six
	000-255
	External mode

	seven
	000-255
	External velocity

	eight
	000-255
	External direction




CH12 channel description:
	passage
	Channel value
	fundamental function

	one
	000-255
	Baiyi

	2
	000-255
	White 2

	three
	000-255
	White 3

	four
	000-255
	R1

	five
	000-255
	G1

	six
	000-255
	B1

	seven
	000-255
	R2

	eight
	000-255
	G2

	nine
	000-255
	B2

	10
	000-255
	R3

	11
	000-255
	G3

	12
	000-255
	B3





CH21 channel description:
	passage
	Channel value
	fundamental function

	one
	000-255
	aiming

	2
	000-255
	stroboscopic

	three
	000-255
	white

	four
	000-255
	White strobe

	five
	000-255
	White mode

	six
	000-255
	White speed

	seven
	000-255
	Inner r

	eight
	000-255
	Neig

	nine
	000-255
	Neib

	10
	000-255
	Internal stroboscopic

	11
	000-255
	Internal mode

	12
	000-255
	Internal velocity

	13
	000-255
	External r

	14
	000-255
	Waig

	151
	000-255
	Waib

	six
	000-255
	External frequency flash

	17
	000-255
	External mode

	18
	000-255
	External velocity

	19
	000-255
	External direction

	20
	000-255
	background color

	21
	000-255
	Background tone light



CH22 channel description:
	passage
	Channel value
	fundamental function

	one
	000-255
	aiming

	2
	000-255
	Baiyi

	three
	000-255
	White 2

	four
	000-255
	White 3

	five
	000-255
	White strobe

	six
	000-255
	White mode

	seven
	000-255
	White speed

	eight
	000-255
	Inner r

	nine
	000-255
	Neig

	10
	000-255
	Neib

	11
	000-255
	Internal stroboscopic

	12
	000-255
	Internal mode

	13
	000-255
	Internal velocity

	14
	000-255
	External r

	151
	000-255
	Waig

	six
	000-255
	Waib

	17
	000-255
	External frequency flash

	18
	000-255
	External mode

	19
	000-255
	External velocity

	20
	000-255
	External direction

	21
	000-255
	background color

	22
	000-255
	Background tone light












CH363 channel description:
	passage
	Channel value
	fundamental function

	one
	000-255
	Baiyi

	2
	000-255
	White 2

	three
	000-255
	White 3

	four
	000-255
	R1

	five
	000-255
	G1

	six
	000-255
	B1

	seven
	000-255
	R2

	eight
	000-255
	G2

	nine
	000-255
	B2

	…
	…
	… …

	361
	000-255
	R120

	362
	000-255
	G120

	363
	000-255
	B120





Seven, technical parameters:
[bookmark: OLE_LINK5]Voltage: AC100~220V 50/60HZ
Control mode: DMX512, self-propelled, master-slave, voice control and RDM function.
Channels: CH06, CH08, CH12, CH21, CH22, CH363.
Dimming: 32bit 0~100% linear dimming
Features: dyeing+flash+auxiliary light
Working temperature: -30 ~50℃
Strobe frequency: 1~30HZ
Appearance: metal, black
Connection mode: DMX512 input/output/power input/output.
IP grade: IP20
Size: weight:
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