811-A407-A410-12颗响尾蛇说明书

1、 [image: ]Display panel and key definition










Menu key: enter/return to the main menu.
Up key: menu function up selection/parameter increment.
Down key: menu function down selection/parameter decreasing.	
Enter key: select the menu function, and confirm and save it when the menu function parameters are modified.
Second, the menu function
After the machine is powered on and reset, press the menu key to enter the main menu (exit after 30 seconds of no operation in the main menu interface). See the main menu menu (5 main menu options in total) for details. Press the Up or Down key to select the main menu, enter the Enter key to modify the function parameters of each menu, and then press the Enter key to save the current function parameters after modification (with power-off memory after saving).
	primary menu
	submenu
	Menu function description

	1. System Settings
	1. DMX address
	Modify the DMX address code up or down (the optional range of address code is 001-512), and press the Enter key to save. The default value is 001.

	
	2. Encoder
	Modify the encoder on/off up or down, save the confirmation key and turn it on by default.

	
	3. X inversion
	Modify the X-reversal on/off up or down, and confirm to save, which is closed by default.

	
	4. Y inversion
	Modify Y-turn on/off up or down, and confirm to save, which is closed by default.

	
	5. Advanced Settings
	

	2. Operation mode
	1. Operation mode
	Select the running mode DMX/ Voice Control/Auto up or down, and press the Enter key to save. The default DMX is selected.

	
	2. Channel selection
	Select up or down channels CH26, CH38, CH62. CH74. CH194 to confirm the key to save. The default is CH26.

	3. Manual control

	1. Y axis
	Modify the parameter value up or down (adjustable range: 000-255), and press the Enter key to save. The default value is 000.

	
	2, y fine-tuning
	Modify the parameter value up or down (adjustable range: 000-255), and press the Enter key to save. The default value is 000.

	
	3, y speed
	Modify the parameter value up or down (adjustable range: 000-255), and press the Enter key to save. The default value is 000.

	
	4, focusing
	Modify the parameter value up or down (adjustable range: 000-255), and press the Enter key to save. The default value is 000.

	
	5. Dimming
	Modify the parameter value up or down (adjustable range: 000-255), and press the Enter key to save. The default value is 000.

	
	6, a strobe
	Modify the parameter value up or down (adjustable range: 000-255), and press the Enter key to save. The default value is 000.

	
	7, a red
	Modify the brightness of the red light bulb up or down (adjustable range 000-255), and press the Enter key to save. The default value is 000.

	
	8, a green
	Modify the brightness of the green light bulb up or down (adjustable range 000-255), and press the Enter key to save. The default value is 000.

	
	9, a blue
	Modify the brightness of the blue light bulb up or down (adjustable range 000-255), and press the Enter key to save. The default value is 000.

	
	10, a white
	Modify the brightness of the white light bulb up or down (adjustable range 000-255), and press the Enter key to save. The default value is 000.

	
	11. Mode A
	Modify the parameter value up or down (adjustable range: 000-255), and press the Enter key to save. The default value is 000.

	
	12, a speed
	Modify the parameter value up or down (adjustable range: 000-255), and press the Enter key to save. The default value is 000.

	
	13, a background color
	Modify the parameter value up or down (adjustable range: 000-255), and press the Enter key to save. The default value is 000.

	
	14, a background color light
	Modify the parameter value up or down (adjustable range: 000-255), and press the Enter key to save. The default value is 000.

	
	15, b strobe
	Modify the parameter value up or down (adjustable range: 000-255), and press the Enter key to save. The default value is 000.

	
	16, b red
	Modify the brightness of the red light bulb up or down (adjustable range 000-255), and press the Enter key to save; the default value is 255.

	
	17, b green
	Modify the brightness of the green light bulb up or down (adjustable range 000-255), and press the Enter key to save; the default value is 255.

	
	18, b blue
	Modify the brightness of the blue bulb up or down (adjustable range 000-255), and press the Enter key to save, and the default value is 255.

	
	19, b white
	Modify the brightness of white light beads up or down (adjustable range 000-255), and press the Enter key to save, and the default value is 255.

	
	20, b yellow
	Modify the brightness of blue and yellow bulbs up or down (adjustable range: 000-255), and press the Enter key to save; the default value is 255.

	
	21. Mode B
	Modify the parameter value up or down (adjustable range: 000-255), and press the Enter key to save. The default value is 000.

	
	22, b speed
	Modify the parameter value up or down (adjustable range: 000-255), and press the Enter key to save. The default value is 000.

	
	23. direction b
	Modify the parameter value up or down (adjustable range: 000-255), and press the Enter key to save. The default value is 000.

	
	24, b background color
	Modify the parameter value up or down (adjustable range: 000-255), and press the Enter key to save. The default value is 000.

	
	25, b background color light
	Modify the parameter value up or down (adjustable range: 000-255), and press the Enter key to save. The default value is 000.

	
	26, reset
	Yes/no

	4. Display settings
	1. Language choice
	Select Chinese /EN (English) up or down, and press the Enter key to save. The default is Chinese.

	
	2. Inverted display settings
	Select up or down to turn off/on the reverse display setting, and press the Enter key to save, which is turned off by default.

	
	3. Screen protection
	Select Close/Open Screen Saver up or down, and confirm to save, which is turned on by default.

	
	4. Software version
	069C program identification code, which cannot be modified.

	5. Factory Settings
	Please enter the password for display! Change it to 138 up or down, and then press the Enter key to enter the factory settings.
	1. Y axis calibration
	Modify the parameter up or down (range 000-255), and confirm to save it. The default value is 128.

	
	
	2, focusing 1 calibration
	Modify the focus 1 calibration (000-255) up or down, and confirm the key to save. The default is 128.

	
	
	3, focusing 2 calibration
	Modify the focus 2 calibration (000-255) up or down, and confirm the key to save. The default is 128.

	
	
	4, focusing stroke
	Modify the focusing stroke (000-255) up or down, and press the Enter key to save. The default value is 128.

	
	
	5. Red
	Modify the red light bulb current (032-255) up or down, and press the Enter key to save. The default value is 252.

	
	
	6. Green
	Modify the green light bulb current up or down (032-255), and press the Enter key to save. The default value is 252.

	
	
	7. Blue
	Modify the blue light bulb current up or down (032-255), and press the Enter key to save. The default value is 252.

	
	
	8. White
	Modify the white light bulb current up or down (032-255), and press the Enter key to save. The default value is 252.

	
	
	9、LEDNum
	Select 000 /0012 up or down, and confirm to save. The default value is 001.

	
	
	10. Current
	Select 000 /007 up or down, and confirm to save. The default value is 004.

	
	
	11. Speed
	Select 000 /007 up or down, and confirm to save. The default value is 000.

	
	
	12、LOGO
	L Select 000 /001 up or down, and confirm to save. The default value is 000.

	
	
	13. Temperature
	Modify the temperature parameter up or down (range 40-70), and confirm to save it. The default value is 065.

	
	
	14. Temperature-Fan
	Select up or down to turn off/on temperature-fan control, and press the Enter key to save and turn it on by default.

	
	
	15、LED
	Select LEDa/ledb in sequence for led lamp beads.

	
	
	16、ETO
	ETO


Third, master-slave control
There are two or more identical lamps connected by DMX three-core signal lines, all lamps are modified to any address code of 001~512, and any one is set as the master, while other lamps are slaves, and all slave displays do not flicker; When the master adjusts the effects of gradual change, pulse change, jump, voice control and self-walking, all slaves synchronize the effects of gradual change, pulse change, jump, voice control and self-walking.
Special attention: 1. Only one host can be set for a group of lamps. If there are multiple hosts, all lamps will flash without synchronization.
2. All lamps and lanterns must be used when the DMX512 console is closed.
Fourth, DMX512 control
Address codes of all lamps and lanterns are set, and all lamps and lanterns are connected to the DMX512 console in parallel with DMX three-core signal lines. The address code stops flashing, indicating that the DMX512 console signal has been sent to the lamps and lanterns. According to the channel description, the DMX512 console is used to control related functions.
CH26 Channel Description:
	passage
	Channel value
	fundamental function

	one
	000-255
	electrical machinery

	2
	000-255
	Motor fine tuning

	three
	000-255
	Motor speed

	four
	000-255
	focus

	five
	000-255
	aiming

	six
	000-255
	Main light stroboscopic

	seven
	000-255
	Main light red

	eight
	000-255
	Main light green

	nine
	000-255
	Main light blue

	10
	000-255
	Main light white

	11
	000-255
	Main light mode

	12
	000-255
	Principal light velocity

	13
	000-255
	Main light background color

	14
	000-255
	Main light background tone light

	15
	000-255
	Auxiliary light strobe

	16
	000-255
	Auxiliary light red

	17
	000-255
	Auxiliary light green

	18
	000-255
	Auxiliary light blue

	19
	000-255
	Auxiliary light white

	20
	000-255
	Auxiliary light yellow

	21
	000-255
	Auxiliary light mode

	22
	000-255
	Auxiliary light speed

	23
	000-255
	Auxiliary light direction

	24
	000-255
	Auxiliary light back scenery

	25
	000-255
	Auxiliary light background tone light

	26
	000-255
	reset



CH38 channel description:
	passage
	Channel value
	fundamental function

	one
	000-255
	electrical machinery

	2
	000-255
	Motor fine tuning

	three
	000-255
	Motor speed

	four
	000-255
	focus

	five
	000-255
	aiming

	six
	000-255
	Main light stroboscopic

	seven
	000-255
	Main light red

	eight
	000-255
	Main light green

	nine
	000-255
	Main light blue

	10
	000-255
	Main light white

	11
	000-255
	Main light mode

	12
	000-255
	Principal light velocity

	13
	000-255
	Main light background color

	14
	000-255
	Main light background tone light

	15
	000-255
	Auxiliary light strobe

	16
	000-255
	Auxiliary light red

	17
	000-255
	Auxiliary light green

	18
	000-255
	Auxiliary light blue

	19
	000-255
	Auxiliary light white

	20
	000-255
	Auxiliary light yellow

	21
	000-255
	Auxiliary light mode

	22
	000-255
	Auxiliary light speed

	23
	000-255
	Auxiliary light direction

	24
	000-255
	Auxiliary light back scenery

	25
	000-255
	Auxiliary light background tone light

	26
	000-255
	reset

	27
	000-255
	Main light LED1

	28
	000-255
	Main light LED2

	29
	000-255
	Main light LED3

	30
	000-255
	Main light LED4

	31
	000-255
	Main light LED5

	32
	000-255
	Main light LED6

	33
	000-255
	Main light LED7

	34
	000-255
	Main light LED8

	35
	000-255
	Main light LED9

	36
	000-255
	Main light LED10

	37
	000-255
	Main light LED11

	38
	000-255
	Main light LED12



CH62 channel description:
	passage
	Channel value
	fundamental function

	one
	000-255
	electrical machinery

	2
	000-255
	Motor fine tuning

	three
	000-255
	Motor speed

	four
	000-255
	focus

	five
	000-255
	aiming

	six
	000-255
	Main light stroboscopic

	seven
	000-255
	Main light red

	eight
	000-255
	Main light green

	nine
	000-255
	Main light blue

	10
	000-255
	Main light white

	11
	000-255
	Main light mode

	12
	000-255
	Principal light velocity

	13
	000-255
	Main light background color

	14
	000-255
	Main light background tone light

	15
	000-255
	Auxiliary light strobe

	16
	000-255
	Auxiliary light red

	17
	000-255
	Auxiliary light green

	18
	000-255
	Auxiliary light blue

	19
	000-255
	Auxiliary light white

	20
	000-255
	Auxiliary light yellow

	21
	000-255
	Auxiliary light mode

	22
	000-255
	Auxiliary light speed

	23
	000-255
	Auxiliary light direction

	24
	000-255
	Auxiliary light back scenery

	25
	000-255
	Auxiliary light background tone light

	26
	000-255
	reset

	27
	000-255
	Main light LED1

	28
	000-255
	Main light LED2

	29
	000-255
	Main light LED3

	30
	000-255
	Main light LED4

	31
	000-255
	Main light LED5

	32
	000-255
	Main light LED6

	33
	000-255
	Main light LED7

	34
	000-255
	Main light LED8

	35
	000-255
	Main light LED9

	36
	000-255
	Main light LED10

	37
	000-255
	Main light LED11

	38
	000-255
	Main light LED12

	39
	000-255
	Auxiliary light LED1

	40
	000-255
	Auxiliary light LED2

	41
	000-255
	Auxiliary light LED3

	forty-two
	000-255
	Auxiliary light LED4

	43
	000-255
	Auxiliary light LED5

	forty-four
	000-255
	Auxiliary light LED6

	45
	000-255
	Auxiliary light LED7

	46
	000-255
	Auxiliary light LED8

	47
	000-255
	Auxiliary light LED9

	48
	000-255
	Auxiliary light LED10

	forty-nine
	000-255
	Auxiliary light LED11

	50
	000-255
	Auxiliary light LED12

	51
	000-255
	Auxiliary light LED13

	fifty-two
	000-255
	Auxiliary light LED14

	53
	000-255
	Auxiliary light LED15

	54
	000-255
	Auxiliary light LED16

	55
	000-255
	Auxiliary light LED17

	fifty-six
	000-255
	Auxiliary light LED18

	57
	000-255
	Auxiliary light LED19

	58
	000-255
	Auxiliary light LED20

	59
	000-255
	Auxiliary light LED21

	60
	000-255
	Auxiliary light LED22

	61
	000-255
	Auxiliary light LED23

	62
	000-255
	Auxiliary light LED24




CH74 channel description:
	passage
	Channel value
	fundamental function

	one
	000-255
	electrical machinery

	2
	000-255
	Motor fine tuning

	three
	000-255
	Motor speed

	four
	000-255
	focus

	five
	000-255
	aiming

	six
	000-255
	Main light stroboscopic

	seven
	000-255
	Main light red

	eight
	000-255
	Main light green

	nine
	000-255
	Main light blue

	10
	000-255
	Main light white

	11
	000-255
	Main light mode

	12
	000-255
	Principal light velocity

	13
	000-255
	Main light background color

	14
	000-255
	Main light background tone light

	15
	000-255
	Auxiliary light strobe

	16
	000-255
	Auxiliary light red

	17
	000-255
	Auxiliary light green

	18
	000-255
	Auxiliary light blue

	19
	000-255
	Auxiliary light white

	20
	000-255
	Auxiliary light yellow

	21
	000-255
	Auxiliary light mode

	22
	000-255
	Auxiliary light speed

	23
	000-255
	Auxiliary light direction

	24
	000-255
	Auxiliary light back scenery

	25
	000-255
	Auxiliary light background tone light

	26
	000-255
	reset

	27
	000-255
	Main light red 1

	28
	000-255
	Main light green 1

	29
	000-255
	Main light blue 1

	30
	000-255
	Main light white 1

	31
	000-255
	Main light red 2

	32
	000-255
	Main light green 2

	33
	000-255
	Main light blue 2

	34
	000-255
	Main light white 2

	35
	000-255
	Main light red 3

	36
	000-255
	Main light green 3

	37
	000-255
	Main light blue 3

	38
	000-255
	Main light white 3

	39
	000-255
	Main light red 4

	40
	000-255
	Main light green 4

	41
	000-255
	Main light blue 4

	forty-two
	000-255
	Main light white 4

	43
	000-255
	Main light red 5

	forty-four
	000-255
	Main light green 5

	45
	000-255
	Main light blue 5

	46
	000-255
	Main light white 5

	47
	000-255
	Main light red 6

	48
	000-255
	Main light green 6

	forty-nine
	000-255
	Main light blue 6

	50
	000-255
	Main light white 6

	51
	000-255
	Main light red 7

	fifty-two
	000-255
	Main light green 7

	53
	000-255
	Main light blue 7

	54
	000-255
	Main light white 7

	55
	000-255
	Main light red 8

	fifty-six
	000-255
	Main light green 8

	57
	000-255
	Main light blue 8

	58
	000-255
	Main light white 8

	59
	000-255
	Main light red 9

	60
	000-255
	Main light green 9

	61
	000-255
	Main light blue 9

	62
	000-255
	Main light white 9

	63
	000-255
	Main light red 10

	64
	000-255
	Main light green 10

	65
	000-255
	Main light blue 10

	66
	000-255
	Main light white 10

	67
	000-255
	Main light red 11

	sixty-eight
	000-255
	Main light green 11

	sixty-nine
	000-255
	Main light blue 11

	70
	000-255
	Main light white 11

	71
	000-255
	Main light red 12

	seventy-two
	000-255
	Main light green 12

	73
	000-255
	Main light blue 12

	74
	000-255
	Main light white 12





CH194 channel description:
	passage
	Channel value
	fundamental function

	one
	000-255
	electrical machinery

	2
	000-255
	Motor fine tuning

	three
	000-255
	Motor speed

	four
	000-255
	focus

	five
	000-255
	aiming

	six
	000-255
	Main light stroboscopic

	seven
	000-255
	Main light red

	eight
	000-255
	Main light green

	nine
	000-255
	Main light blue

	10
	000-255
	Main light white

	11
	000-255
	Main light mode

	12
	000-255
	Principal light velocity

	13
	000-255
	Main light background color

	14
	000-255
	Main light background tone light

	15
	000-255
	Auxiliary light strobe

	16
	000-255
	Auxiliary light red

	17
	000-255
	Auxiliary light green

	18
	000-255
	Auxiliary light blue

	19
	000-255
	Auxiliary light white

	20
	000-255
	Auxiliary light yellow

	21
	000-255
	Auxiliary light mode

	22
	000-255
	Auxiliary light speed

	23
	000-255
	Auxiliary light direction

	24
	000-255
	Auxiliary light back scenery

	25
	000-255
	Auxiliary light background tone light

	26
	000-255
	reset

	27
	000-255
	Main light red 1

	28
	000-255
	Main light green 1

	29
	000-255
	Main light blue 1

	30
	000-255
	Main light white 1

	31
	000-255
	Main light red 2

	32
	000-255
	Main light green 2

	33
	000-255
	Main light blue 2

	34
	000-255
	Main light white 2

	35
	000-255
	Main light red 3

	36
	000-255
	Main light green 3

	37
	000-255
	Main light blue 3

	38
	000-255
	Main light white 3

	39
	000-255
	Main light red 4

	40
	000-255
	Main light green 4

	41
	000-255
	Main light blue 4

	forty-two
	000-255
	Main light white 4

	43
	000-255
	Main light red 5

	forty-four
	000-255
	Main light green 5

	45
	000-255
	Main light blue 5

	46
	000-255
	Main light white 5

	47
	000-255
	Main light red 6

	48
	000-255
	Main light green 6

	forty-nine
	000-255
	Main light blue 6

	50
	000-255
	Main light white 6

	51
	000-255
	Main light red 7

	fifty-two
	000-255
	Main light green 7

	53
	000-255
	Main light blue 7

	54
	000-255
	Main light white 7

	55
	000-255
	Main light red 8

	fifty-six
	000-255
	Main light green 8

	57
	000-255
	Main light blue 8

	58
	000-255
	Main light white 8

	59
	000-255
	Main light red 9

	60
	000-255
	Main light green 9

	61
	000-255
	Main light blue 9

	62
	000-255
	Main light white 9

	63
	000-255
	Main light red 10

	64
	000-255
	Main light green 10

	65
	000-255
	Main light blue 10

	66
	000-255
	Main light white 10

	67
	000-255
	Main light red 11

	sixty-eight
	000-255
	Main light green 11

	sixty-nine
	000-255
	Main light blue 11

	70
	000-255
	Main light white 11

	71
	000-255
	Main light red 12

	seventy-two
	000-255
	Main light green 12

	73
	000-255
	Main light blue 12

	74
	000-255
	Main light white 12

	75
	000-255
	Auxiliary light red 1

	76
	000-255
	Auxiliary light green 1

	77
	000-255
	Auxiliary light blue 1

	seventy-eight
	000-255
	Auxiliary light white 1

	79
	000-255
	Auxiliary light yellow 1

	80
	000-255
	Auxiliary light red 2

	81
	000-255
	Auxiliary light green 2

	82
	000-255
	Auxiliary light blue 2

	83
	000-255
	Auxiliary light white 2

	84
	000-255
	Auxiliary light yellow 2

	eighty-five
	000-255
	Auxiliary light red 3

	86
	000-255
	Auxiliary light green 3

	87
	000-255
	Auxiliary light blue 3

	88
	000-255
	Auxiliary light white 3

	eighty-nine
	000-255
	Auxiliary light yellow 3

	90
	000-255
	Auxiliary light red 4

	91
	000-255
	Auxiliary light green 4

	92
	000-255
	Auxiliary light blue 4

	93
	000-255
	Auxiliary light white 4

	94
	000-255
	Auxiliary light yellow 4

	95
	000-255
	Auxiliary light red 5

	96
	000-255
	Auxiliary light green 5

	97
	000-255
	Auxiliary light blue 5

	98
	000-255
	Auxiliary light white 5

	99
	000-255
	Auxiliary light yellow 5

	100
	000-255
	Auxiliary light red 6

	101
	000-255
	Auxiliary light green 6

	102
	000-255
	Auxiliary light blue 6

	103
	000-255
	Auxiliary light white 6

	104
	000-255
	Auxiliary light yellow 6

	105
	000-255
	Auxiliary light red 7

	106
	000-255
	Auxiliary light green 7

	107
	000-255
	Auxiliary light blue 7

	108
	000-255
	Auxiliary light white 7

	109
	000-255
	Auxiliary light yellow 7

	110
	000-255
	Auxiliary light red 8

	111
	000-255
	Auxiliary light green 8

	112
	000-255
	Auxiliary light blue 8

	113
	000-255
	Auxiliary light white 8

	114
	000-255
	Auxiliary light yellow 8

	115
	000-255
	Auxiliary light red 9

	116
	000-255
	Auxiliary light green 9

	117
	000-255
	Auxiliary light blue 9

	118
	000-255
	Auxiliary light white 9

	119
	000-255
	Auxiliary light yellow 9

	120
	000-255
	Auxiliary light red 10

	121
	000-255
	Auxiliary light green 10

	122
	000-255
	Auxiliary light blue 10

	123
	000-255
	Auxiliary light white 10

	124
	000-255
	Auxiliary light yellow 10

	125
	000-255
	Auxiliary light red 11

	126
	000-255
	Auxiliary light green 11

	127
	000-255
	Auxiliary light blue 11

	128
	000-255
	Auxiliary light white 11

	129
	000-255
	Auxiliary light yellow 11

	130
	000-255
	Auxiliary light red 12

	131
	000-255
	Auxiliary light green 12

	132
	000-255
	Auxiliary light blue 12

	133
	000-255
	Auxiliary light white 12

	134
	000-255
	Auxiliary light yellow 12

	135
	000-255
	Auxiliary light red 13

	136
	000-255
	Auxiliary light green 13

	137
	000-255
	Auxiliary light blue 13

	138
	000-255
	Auxiliary light white 13

	139
	000-255
	Auxiliary light yellow 13

	140
	000-255
	Auxiliary light red 14

	141
	000-255
	Auxiliary light green 14

	142
	000-255
	Auxiliary light blue 14

	143
	000-255
	Auxiliary light white 14

	144
	000-255
	Auxiliary light yellow 14

	145
	000-255
	Auxiliary light red 15

	146
	000-255
	Auxiliary light green 15

	147
	000-255
	Auxiliary light blue 15

	148
	000-255
	Auxiliary light white 15

	149
	000-255
	Auxiliary light yellow 15

	150
	000-255
	Auxiliary light red 16

	151
	000-255
	Auxiliary light green 16

	152
	000-255
	Auxiliary light blue 16

	153
	000-255
	Auxiliary light white 16

	154
	000-255
	Auxiliary light yellow 16

	155
	000-255
	Auxiliary light red 17

	156
	000-255
	Auxiliary light green 17

	157
	000-255
	Auxiliary light blue 17

	158
	000-255
	Auxiliary light white 17

	159
	000-255
	Auxiliary light yellow 17

	160
	000-255
	Auxiliary light red 18

	161
	000-255
	Auxiliary light green 18

	162
	000-255
	Auxiliary light blue 18

	163
	000-255
	Auxiliary light white 18

	164
	000-255
	Auxiliary light yellow 18

	165
	000-255
	Auxiliary light red 19

	166
	000-255
	Auxiliary light green 19

	167
	000-255
	Auxiliary light blue 19

	168
	000-255
	Fuguangbai 19

	169
	000-255
	Auxiliary light yellow 19

	170
	000-255
	Auxiliary light red 20

	171
	000-255
	Auxiliary light green 20

	172
	000-255
	Auxiliary light blue 20

	173
	000-255
	Auxiliary light white 20

	174
	000-255
	Auxiliary light yellow 20

	175
	000-255
	Auxiliary light red 21

	176
	000-255
	Auxiliary light green 21

	177
	000-255
	Auxiliary light blue 21

	178
	000-255
	Auxiliary light white 21

	179
	000-255
	Auxiliary light yellow 21

	one hundred and eighty 
	000-255
	Auxiliary light red 22

	181
	000-255
	Auxiliary light green 22

	182
	000-255
	Auxiliary light blue 22

	183
	000-255
	Auxiliary light white 22

	184
	000-255
	Auxiliary light yellow 22

	185
	000-255
	Auxiliary light red 23

	186
	000-255
	Auxiliary light green 23

	187
	000-255
	Auxiliary light blue 23

	188
	000-255
	Auxiliary light white 23

	189
	000-255
	Auxiliary light yellow 23

	190
	000-255
	Auxiliary light red 24

	191
	000-255
	Auxiliary light green 24

	192
	000-255
	Auxiliary light blue 24

	193
	000-255
	Auxiliary light white 24

	194
	000-255
	Auxiliary light yellow 24







V. Technical parameters:
[bookmark: OLE_LINK5]Voltage: AC100~240V 50/60HZ
Power: 500W
Lamp beads: 12 40W four-in-one foot Tim Xin lamp beads 144 0.3W 5050 three-in-one lamp beads.
Control mode: DMX512, self-propelled, master-slave, voice control and RDM function.
Channels: CH26, CH38, ch62.ch74.ch194.
Dimming: 32bit 0~100% linear dimming
Features: Y shake head+beam+flash+auxiliary light.
Working temperature: -30 ~50℃
Strobe frequency: 1~30HZ
Appearance: metal, black
Connection mode: DMX512 input/output/power input/output.
IP grade: IP20
Size:
[bookmark: _GoBack] weight:
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