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	MENU: Select the function mode or return to the previous menu.
	
	

	UP: select up
	
	

	DOWN: select down.
	
	

	ENTER: confirm
	
	



	Technical parameters:
Voltage: AC100~240V 50/60HZ
Power: 180W.

	Lamp beads: 441pcs 5050RGB(0.25w) +49pcs 5730U(5w)
Control mode: DMX512,Auto, master-slave, voice control, with RDM function.

	Channels: CH4, CH13 and CH14

	Linear dimming features: 441RGB+49W single point control.

	Working temperature: -30 ~50℃

	Strobe frequency: 1~30HZ

	Connection mode: DMX512 input/output/power input/output
IP grade: IP20.

	Primary menu
	Sub menu 1
	Sub menu 2
	Remarks

	Address
	D001/D512
	
	Address code, press enter key to enter sub menu 1, press up key or down key to select the address code, and press enter key to save the address code.

	CHAL
	CH5、CH13、CH14
	
	Channel, press OK to enter sub menu 1, press the up key or the down key to select the channel, and press OK to save the channel.

	AUTO
	CA50
	01-50
	Press the Enter key to enter the second level, press the Up key or the Down key to select the self-propelled effect (254 kinds of effects), and then press the Enter key to enter the third level. The third level menu includes: s00-s50 speed, c000-c255 color (most effects support 255 color styles, and the unsupported effect is that the interval value switches different original colors). In the third level menu, press the Enter key to switch between speed and color and save the self-propelled type and speed, and press.

	
	CB50
	01-50
	

	
	CC50
	01-50
	

	
	CD50
	01-50
	

	
	CE50
	01-50
	

	
	CF50
	01-50
	

	
	CG50
	01-50
	

	
	CH50
	01-50
	

	
	CJ50
	01-50
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	SOUD
	SO01-SO99
	
	Voice control mode secondary menu: A00-A99 Sensitivity effect N000-N254

	STAT
	r000
	r000-r255
	Red manual dimming

	
	g000
	g000-g255
	Green manual dimming

	
	b000
	b000-b255
	Blue manual dimming

	
	w000
	w000-w255
	White manual dimming

	
	c000
	c000-c094
	character

	
	d000
	d000-d003
	direction

	
	t000
	t000-b255
	stroboscopic

	Rest
	On/Off
	
	Restore factory settings






	backstage
	
	

	r000
	r000-r255
	Power adjustment of red lamp bead

	g000
	g000-g255
	Power adjustment of green lamp bead

	b000
	b000-b255
	Power adjustment of blue lamp bead

	w000
	w000-w255
	White light bulb power adjustment

	n000
	n000-n255
	Reduce power

	l000
	l000-l255
	Maximum rate

	OFF
	OFF/ON
	send



	Channel 4
	Channel value
	fundamental function
	

	1
	000-255
	R red light bulb dimming
	

	2
	000-255
	G green light bulb dimming
	

	3
	000-255
	B blue light bulb dimming
	

	4
	000-255
	W white light bulb dimming
	

	
	
	
	

	Channel 13
	Channel value
	fundamental function
	

	1
	000-255
	Total dimming
	

	2
	000-255
	stroboscopic
	

	3
	000-255
	Position lever
	

	4
	000-255
	Color bar
	

	5
	000-255
	Effect, 255 is voice control
	

	6
	000-255
	speed
	

	7
	000-255
	White light flashing
	

	8
	000-255
	White light effect
	

	9
	000-255
	White light speed
	

	10
	000-255
	R red light bulb dimming
	

	11
	000-255
	G green light bulb dimming
	

	12
	000-255
	B blue light bulb dimming
	

	13
	000-255
	W white light bulb dimming
	

	
	
	
	

	
	
	
	

	Channel 14
	Channel value
	fundamental function
	

	1
	000-255
	Total dimming
	

	2
	000-255
	stroboscopic
	

	3
	000-255
	direction
	

	4
	000-255
	Color/style
	

	5
	000-255
	Translation (0-200), automatic left translation (200-225), automatic right translation (225-255)
	Note: After turning on the general dimming, you can complete the 
writing of words only by operating the No.5 and No.6 levers.
After writing, push the No.5 rod to more than 200, and then you can 
pan and display the content written by it.

	6
	000-255
	Letter/number/symbol selection
	

	7
	000-255
	speed
	

	8
	000-255
	Auxiliary lamp stroboscopic
	

	9
	000-255
	Auxiliary lamp effect
	

	10
	000-255
	Auxiliary lamp speed
	

	11
	000-255
	R red light bulb dimming
	

	12
	000-255
	G green light bulb dimming
	

	13
	000-255
	B blue light bulb dimming
	

	14
	000-255
	W white light bulb dimming
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