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(Please read the instructions carefully and manage them properly before using the product)








In order to use this product correctly and safely, please read the instructions carefully before installing and using this product. This manual contains important installation and application information. Please strictly follow the instructions when installing and operating the product. At the same time, please keep this manual properly.
Our company's  beam lamp A new beautiful high-temperature-resistant metal body is used. This product is designed and produced in strict accordance with CE standards. It conforms to the international standard DMX512 signal protocol. It can be used alone or online. It has the characteristics of fast rotation, low noise and powerful functions. It is suitable for small and medium-sized concerts, theaters, studios, nightclubs, bars and other places.
Please carefully remove the packaging, check whether the product is damaged during transportation after the packaging is removed, and check whether the following contents are complete. 。       
          
Beam lamp--------1 instruction manual--------1 book
          Power cord--------1 signal line--------1                 
This product is in good condition before leaving the factory. In order to keep the product in good condition and ensure safe operation, users should follow the safety matters and the warnings in this manual.
Important:Damage caused by non-compliance with this manual is not covered by the warranty. The supplier is not responsible for the resulting product problems.
If the product has been exposed to an extremely unstable temperature environment (such as after transportation), please do not connect the product to the power supply immediately, because water droplets caused by temperature changes may damage the product. Please use it after the product returns to normal temperature. 
[bookmark: _GoBack]This product can Used in the AC110-240V voltage range, it is a product for indoor use. Please make sure that the voltage used is not higher than the range that the product can withstand!! The power plug must be plugged into a protective I.Kind of socket. The green or tea-blue conductor must be grounded.
Please check this product and power cord frequently. Make sure that the power cord is not folded or scratched, and is not connected to other cables! Special attention should be paid when connecting the power cord or related connection. Be sure to unplug the power supply when not using this product or before cleaning. 
Before using the product, please familiarize yourself with the operation function of the product. Please do not expose children or non-professionals to the product. Please do not shake this product. Do not use brute force when installing or operating products. Don't let non-professionals operate the product. Most of the damage is caused by unprofessional operation. 
The product is not equipped with relevant repair accessories. The maintenance and repair of products can only be carried out by professionals! 
Please do not change this product without authorization, otherwise it may damage the product, so the damage caused is not covered by the warranty. Moreover, unprofessional operation may lead to short circuit, burn or electric shock, etc.




Connection of DMX512 signal:
This lamp uses DMX512 signal control mode. The control signal of each lamp is in parallel. When connecting multiple lamp signals, it is best to use a double-core shielded cable. When connecting, each lamp is connected through the DMX signal jack (Canon seat) INPUT (input) and OUTPUT (output) on the lamp. The 3-core XLR plug terminal connecting the signal line of the lamp must correspond to each other. When connecting the lamp signal, it is recommended to use the DMX signal terminal. . It can be avoided that the control signal is damaged due to electrical noise. The DMX signal terminal connects a 120 ohm 1W resistor between the 2 pins and 3 pins of an XLR plug and connects it to the OUTPUT (output) jack of the last lamp.
Calculation method of the starting address code of the lamp:
The starting address code of the current lamp is equal to (the starting address code of the previous lamp) + (the number of channels of the lamp) Description:
1: The starting address value of the first lamp is A001. 
2: The basic number of channels of the controller should be greater than or equal to the total number of channels used by the lamp. 
3: Note: When using any controller, each lamp must have its own starting address code. If the starting address code of the first lamp is set to A001 and the number of lamp channels is 16CH; then the starting address code of the second lamp is set to A01. 7The starting address code of the third lamp is set to A03.3By analogy, (this setting also needs to be determined according to different consoles).






	menu operation settings

	Main menu
	Sub-menu one
	Function settings
	Introduction to functions

	DMX address
	
	1-512
	

	System settings
	Show inverted 
	Normal
	.

	
	
	Flip over
	

	
	Language settings 
	Chinese
	

	
	
	English
	

	
	Channel mode 
	20CH
	

	
	Operation mode 
	DMX 
	

	
	
	Sound-activated
	

	
	
	Voluntary
	

	
	Electronic lighting 
	Shut
	

	
	
	Open
	

	
	The light bulb defaults 
	Open_Close
	

	
	Light bulb control 
	Light up. 
	

	
	The shortest path 
	Open_Close
	

	
	Horizontal reverse 
	Shut
	

	
	
	Open
	

	
	Vertical and reverse 
	Shut
	

	
	
	Open
	

	
	XY speed 
	Low speed
	

	
	
	Medium speed
	

	
	
	Fast
	

	
	Optocoupler detection 
	Shut
	

	
	
	Open
	

	
	Return to the superior 
	▲
	

	Information inquiry 
	Total time 
	0-9999
	

	
	Light bulb time 
	0-9999
	

	
	Time limit 
	0-9999
	

	
	Display software 
	Vx001
	

	
	XY software 
	Vx001
	

	
	Small motor software
	Vx001
	

	
	Return to the superior 
	▲
	

	Channel control 
	Rotation of the color palette
	0-255
	

	
	Strobe 
	0-255
	

	
	Dim the light
	0-255
	

	
	Fixed pattern 
	0-255
	

	
	Prism 
	0-255
	

	
	Prism rotation.
	0-255
	

	
	Atomization 
	0-255
	

	
	Focusing. 
	0-255
	

	
	Horizontal rotation 
	0-255
	

	
	Horizontal fine-tuning 
	0-255
	

	
	Vertical rotation 
	0-255
	

	
	Vertical fine-tuning 
	0-255
	

	
	Reduce 
	0-255
	

	
	Light up 
	0-255
	

	
	XY speed 
	0-255
	

	
	Color disk speed 
	0-255
	

	
	Focusing speed 
	0-255
	

	
	Pattern speed 
	0-255
	

	
	Return to the superior
	0-255
	

	Working status 
	XY communication 
	Normal
	Current status

	
	
	Wrong
	

	
	Small motor communication
	Normal
	

	
	
	Wrong
	

	
	Focusing Hall 
	Normal
	

	
	
	Wrong
	

	
	Color plate Hall 
	Normal
	

	
	
	Wrong
	

	
	Pattern Hall 
	Normal
	

	
	
	Wrong
	

	
	X-optical coupling 
	Normal
	

	
	
	Wrong
	

	
	Y optocoupler 
	Normal
	

	
	
	Wrong
	

	
	Fan speed. 
	6500
	

	
	Return to the superior 
	▲
	

	Auxiliary tools 
	Check code 1 
	0-9999
	

	
	Total time 
	Reset
	

	
	
	Carry out
	

	
	Light and cannon time 
	Reset
	

	
	
	Carry out
	

	
	Restore the default 
	Tacitly approve
	

	
	
	Resume
	

	
	
	Preserve
	

	
	Horizontal rotation 
	0-255
	Zero initial position

	
	Vertical rotation 
	0-255
	

	
	Focusing. 
	0-255
	

	
	Prism 1 (the prism) 
	0-255
	

	
	Prism 2 (Skiw) 
	0-255
	

	
	Prism rotation 1st 
	0-255
	

	
	Prism rotation 2 (two) 
	0-255
	

	
	Atomization 
	0-255
	

	
	Color combination 
	0-255
	

	
	Fixed pattern 
	0-255
	

	
	Color plate 
	0-255
	

	
	Strobes 
	0-255
	

	
	The midpoint of strobe 
	0-255
	

	
	The middle point of the first point 
	0-255
	

	
	The middle point of the two edges 
	0-255
	

	
	Midpoint of atomization 
	0-255
	

	
	Colorful points 
	0-255
	

	
	Return to the superior 
	▲
	

	Advanced settings 
	Check code 2 
	0-9999
	

	
	Encryption of signals 
	Open
	

	
	
	Shut
	

	
	DMX speed 
	0-255
	

	
	DMX data package 
	0-255
	

	
	DMX type 
	0-055
	

	
	DMX isolation 
	0-65535
	The smaller the value, the more stable the signal.

	
	Drive board temperature
	<110 degrees>
	If it exceeds this range, it will show red.

	
	Drive board 3.3V
	3.0V - 3.6V
	If it exceeds this range, it will show red.

	
	Drive board 5.0V
	4.5V - 5.5V
	If it exceeds this range, it will show red.

	
	Drive board 12V 
	10.0V - 14.0V
	If it exceeds this range, it will show red.

	
	Drive board 36V 
	20.0V - 42.0V
	If it exceeds this range, it will show red.

	
	X state 
	Be static 
	

	
	
	Turn 
	

	
	X Hall 
	Normal 
	

	
	
	Wrong 
	Show red

	
	X-coupler phase 
	0-3
	

	
	X-coupler A 
	40-160
	The standard setting of 100 exceeds the required range to display red, but the red light on the panel does not alarm.

	
	X-optical coupling B 
	40-160
	The standard setting of 100 exceeds the required range to display red, but the red light on the panel does not alarm.

	
	X-optical coupling C 
	40-160
	The standard setting of 100 exceeds the required range to display red, but the red light on the panel does not alarm.

	
	X-optical coupling D 
	40-160
	The standard setting of 100 exceeds the required range to display red, but the red light on the panel does not alarm.

	
	X current angle 
	000-540
	

	
	X-driven state 
	Normal 
	

	
	
	Wrong 
	Show red

	
	Y state 
	Be static 
	

	
	
	Turn 
	

	
	Y optocoupler 
	Normal 
	

	
	
	Wrong 
	Show red

	
	Y Hall 
	Normal 
	

	
	
	Wrong 
	Show red

	
	Y photocoupler phase 
	0-3
	

	
	Y optocoupler A 
	40-160
	If it exceeds this range, it will show red.

	
	Y optocoupler B 
	40-160
	If it exceeds this range, it will show red.

	
	Y optocoupler C 
	40-160
	If it exceeds this range, it will show red.

	
	Y optocoupler D 
	40-160
	If it exceeds this range, it will show red.

	
	Y current angle 
	000-250
	

	
	Y drive state 
	Normal 
	

	
	
	Wrong 
	Show red

	
	Return to the superior 
	▲
	

	Channel level. 
	Rotation of the color palette 
	0-255
	Current DMX channel value

	
	Strobe 
	0-255
	

	
	Dim the light 
	0-255
	

	
	Fixed pattern 
	0-255
	

	
	Prism 
	0-255
	

	
	Prism rotation.
	0-255
	

	
	Atomization 
	0-255
	

	
	Focusing. 
	0-255
	

	
	Horizontal rotation 
	0-255
	

	
	Horizontal fine-tuning 
	0-255
	

	
	Vertical rotation 
	0-255
	

	
	Vertical fine-tuning 
	0-255
	

	
	Reduce 
	0-255
	

	
	Light up 
	0-288
	

	
	XY speed 
	0-255
	

	
	Color disk speed 
	0-255
	

	
	Focusing speed 
	0-255
	

	
	Pattern speed 
	0-255
	

	
	Return to the superior 
	
	

	Reduce 
	Re-re reset all 
	Cancel
	Manual reset.

	
	
	Carry out
	

	
	XY reset 
	Cancel
	

	
	
	Carry out
	

	
	Effect reset "
	Cancel
	

	
	
	Carry out
	

	
	Return to the superior 
	
	

	Exit the menu 
	
	
	



●20Channel table
	Passageway
	Name
	Numerical value
	Describe

	CH1
	CH1
	Color
	0-4
	White light

	
	
	
	5-9
	White light + color 1

	
	
	
	10-14
	Color1

	
	
	
	15-19
	Color1+Color 2

	
	
	
	20-24
	Color2

	
	
	
	25-29
	Color2+Color3

	
	
	
	30-34
	Color3

	
	
	
	35-39
	Color3+Color4

	
	
	
	40-44
	Color4

	
	
	
	45-49
	Color4+Color5

	
	
	
	50-54
	Color5

	
	
	
	55-59
	Color5+Color6

	
	
	
	60-64
	Color6

	
	
	
	65-69
	Color6+Color7

	
	
	
	70-74
	Color7

	
	
	
	75-79
	Color7+Color8

	
	
	
	80-84
	Color8

	
	
	
	85-89
	Color8+ Color9 

	
	
	
	90-94
	Color9 

	
	
	
	95-99
	Color9+ Color 10 

	
	
	
	100-104
	Color10 

	
	
	
	105-109
	Color10+ Color 11

	
	
	
	110-114
	Color11

	
	
	
	115-119
	Color11+ Color 12

	
	
	
	120-124
	Color12 

	
	
	
	125-129
	Color12+ Color 13

	
	
	
	130-134
	Color13 

	
	
	
	135-139
	Color 13  + White light 

	
	
	
	140-149
	White light 

	
	
	
	150-203
	From fast to slow, forward flowing water

	
	
	
	204-255
	Reverse flow from slow to fast

	CH2
	CH2
	Strobe
	0-3
	The light gate is closed.

	
	
	
	4-103
	Synchronous strobe

	
	
	
	104-107
	The light gate opens.

	
	
	
	108-207
	Divide the strobe equally.

	
	
	
	208-212
	The light gate opens.

	
	
	
	213-225
	Low-speed random strobe

	
	
	
	226-238
	Medium-speed random strobe

	
	
	
	239-251
	High-speed random strobe

	
	
	
	252-255
	The light gate opens.

	CH3
	CH3
	Dim the light
	0-255
	0-100% dimming

	CH4
	CH4
	Pattern
	0-3
	White light hole

	
	
	
	4-7
	Pattern 1

	
	
	
	8-11
	Pattern 2

	
	
	
	12-15
	Pattern 3

	
	
	
	16-19
	Pattern 4

	
	
	
	20-23
	Pattern 5

	
	
	
	24-27
	Pattern 6

	
	
	
	28-31
	Pattern 7

	
	
	
	32-35
	Pattern 8

	
	
	
	36-39
	Pattern 9

	
	
	
	40-43
	Pattern 10

	
	
	
	44-47
	Pattern 11

	
	
	
	48-51
	Pattern 12

	
	
	
	52-55
	Pattern13

	
	
	
	56-59
	Pattern14

	
	
	
	60-63
	Pattern15

	
	
	
	64-67
	Pattern16

	
	
	
	68-71
	Pattern17

	
	
	
	72-111
	Forward rotation-Fast-slow

	
	
	
	112-115
	Stop the running water

	
	
	
	1116-155
	Reverse rotation- Slow - Fast

	
	
	
	156-161
	Pattern1From slow to fast jitter

	
	
	
	162-167
	Pattern 2 shakes from slow to fast

	
	
	
	168-173
	Pattern 3 from slow to fast jitter

	
	
	
	174-179
	Pattern 4 from slow to fast jitter

	
	
	
	180-185
	Pattern5From slow to fast jitter

	
	
	
	186-191
	Pattern6From slow to fast jitter

	
	
	
	192-197
	Pattern7From slow to fast jitter

	
	
	
	198-203
	Pattern8From slow to fast jitter

	
	
	
	204-209
	Pattern9From slow to fast jitter

	
	
	
	210-216
	Pattern10From slow to fast jitter

	
	
	
	217-222
	Pattern11From slow to fast jitter

	
	
	
	223-228
	Pattern12From slow to fast jitter

	
	
	
	229-234
	Pattern13From slow to fast jitter

	
	
	
	235-240
	Pattern 14From slow to fast jitter

	
	
	
	241-246
	Pattern 15From slow to fast jitter

	
	
	
	247-252
	Pattern 16From slow to fast jitter

	
	
	
	253-255
	Pattern 17From slow to fast jitter

	CH5
	CH5
	Prism
	0-127
	Remove the prism.

	
	
	
	128-255
	Prism cut in

	CH6
	CH6
	Prism rotation.
	0-127
	0-400 degrees

	
	
	
	128-190
	From fast to slowTurn overFlowing water

	
	
	
	191-192
	Stop

	
	
	
	193-255
	From slow to fastFirst month of the lunar yearFlowing water

	
	
	
	
	

	CH7
	CH7
	Reserve
	0-255
	No function

	CH8
	CH8
	Colorful atomization
	0-127
	Not have

	
	
	
	128-192
	Insert atomization

	
	
	
	193-255
	Insert seven colors

	CH9
	CH9
	Focus on
	0-255
	From far to near

	CH10
	CH10
	X axis
	0-255
	0-540Linear measure

	CH11
	CH11
	X-axis fine-tuning
	0-255
	UnknownAxis 16Bit fine-tuning channel

	CH12
	CH12
	Y-axis
	0-255
	0-240 degrees

	CH13
	CH13
	Y-axis fine-tuning
	0-255
	Y-axis 16Bit fine-tuning channel

	CH14
	CH14
	Reserve
	0-255
	No function

	
CH15
	CH15
	Reduce
	0-25
	No function

	
	
	
	26-76
	Effect motor reset (5S)

	
	
	
	77-127
	Scanning motor reset (5S)

	
	
	
	128-255
	All motor reset (5S)

	
CH16
	CH16
	Reduce
	0-9
	No function

	
	
	
	10-100
	Extinguish the light bulb (5S)

	
	
	
	101-255
	Light bulb (5S)

	
	CH17
	XY speed
	0-255
	From fast to slow

	
	CH18
	Color disk speed
	0-255
	From fast to slow

	
	CH19
	Prism atomization speed
	0-255
	From fast to slow

	
	CH20
	Pattern disk speed
	0-255
	From fast to slow




Installation instructions for lamps and lanterns:
This lamp can be placed horizontally, hanging obliquely and upside down. You must pay attention to the installation method when hanging obliquely and upside down. Fixed installation of lamps and lanterns: Before positioning the lamps and lanterns, it is necessary to ensure the stability of the installation site. When reverting the hanging installation, it is necessary to ensure that the lamps and lanterns do not fall off the support frame. The safety rope should be used to pierce the support frame and the lamp handle to carry out auxiliary hanging to ensure safety. To prevent the lamp from falling and sliding, when the lamp is installed and debugged, pedestrians are prohibited from passing through the lower part. Regularly check whether the safety rope is worn and whether the hook screw is loose. If the hanging installation is unstable, the manufacturer shall not bear any responsibility for all the consequences caused by the falling of the lamp.


After-sales service
Attention! When the lamps leave the factory, they have undergone strict quality inspection and the packaging is intact. Please follow the instructions. Machine failures caused by human causes are not covered by the warranty. 
1. The company provides technical consultation to customers throughout their lives.
2. If the product fails and needs to be repaired, please show the product warranty card and fill in the relevant content truthfully. At the same time, we also hope that customers can give us feedback on the problems of the product in time, so that we can improve the product as soon as possible.
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