Instructions for 24 Thunder Curtain Lights



















Because the products are constantly updated, the contents of this manual may be slightly different from the actual products, please understand!



product catalog
1、 Display panel key function
2、 Menu function description
3、 Channel description
4、 Use of common functions
5， Master-slave setting
6， technical parameter
One: Display panel operation
[image: ]
Menu up and down confirmation
Basic usage:
MENU key: select various functions.
UP: Incremental selection of function parameters.
DOWN: function parameters are selected in descending order.
ENTER: determines the current menu.

Second, the menu function
Press the MENU key (menu key) after power-on and start-up, and the following functions will appear in turn, and then press the confirm key to confirm. (This order is the new machine order. If the lamp has used other modes and saved this mode before turning off, the mode before turning off will be displayed after turning on again.) After setting other functions, you also need to press the Save button to save, otherwise the effect of setting before turning off will not appear after turning on next time.
	A001
	
	001-512
	address code

	10CH
	Channel mode
	
	Channel selection 05CH,10CH,128CH,138CH.

	-512
	operational mode
	
	DMX512, voice control, self-propelled

	E001
	Effect mode
	E001-E250
	Effect selection (250 kinds)

	P000
	Effect speed
	P000-P255
	The UP/DOWN key selects the running speed (P000-P255), and the ENTER key saves the current running speed.

	CL00
	Effect color selection
	CL00-CL07
	7 color choices

	R255
	Manual red
	R000-R255
	Manual red adjustment, when there is no console, use the UP/DOWN key to adjust the brightness between R000 and R255.

	G255
	Manual green
	G000-G255
	Manual green adjustment, when there is no console, use the UP/DOWN key to adjust the brightness between G000 and G255.

	B255
	Manual blue
	B000-B255
	Manual blue adjustment, when there is no console, use the UP/DOWN key to adjust the brightness between B000 and B255.

	W255
	Manual white light
	W000-W255
	Manual white light adjustment, when there is no console, use UP/DOWN key to adjust brightness between W000 and W255.

	Y255
	Manual cold white light
	Y000-Y255
	Manual cold white light adjustment, when there is no console, use the UP/DOWN key to adjust the brightness between Y000 and Y255.

	F000
	Manual stroboscopic
	F000-F255
	Use the UP or DOWN key to select the strobe speed.

	T000
	Temperature display
	T000-T105
	Display temperature

	Press the OK key to save after setting, and the display will flash when saving.



3， Channel description
	5 channels
	function
	Channel value
	describe

	one
	Red (r)
	0-255
	0-%100 linear dimming

	2
	Green (g)
	0-255
	0-%100 linear dimming

	three
	Blue (b)
	0-255
	0-%100 linear dimming

	four
	White (w)
	0-255
	0-%100 linear dimming

	five
	Cold white (y)
	0-255
	0-%100 linear dimming


	10 channels
	function
	Channel value
	describe

	one
	Total dimming
	0-255
	0-%100 linear dimming

	2
	stroboscopic
	0-9
	neutrality

	
	
	10-255
	Strobe from slow to fast

	three
	Combined effect
	0
	all-or-none

	
	
	one
	R

	
	
	2
	G

	
	
	three
	B

	
	
	four
	RG

	
	
	five
	RB

	
	
	six
	GB

	
	
	seven
	RGB

	
	
	eight
	W

	
	
	nine
	Y

	
	
	10
	RGBWY

	
	
	11
	gradual change

	
	
	12
	Pulse change

	
	
	13
	jump

	
	
	14
	Effect 1

	
	
	…
	…

	
	
	250
	Effect 237

	
	
	251-255
	sound-controlled

	four
	Combined effect speed
	0-255
	Speed from slow to fast

	five
	Combination effect color selection
	0-15
	be invalid

	
	
	16-50
	R

	
	
	51-85
	G

	
	
	86-120
	B

	
	
	121-155
	RG

	
	
	156-190
	RB

	
	
	191-225
	GB

	
	
	226-255
	RGB

	six
	Red (r)
	0-255
	0-%100 linear dimming

	seven
	Green (g)
	0-255
	0-%100 linear dimming

	eight
	Blue (b)
	0-255
	0-%100 linear dimming

	nine
	White (w)
	0-255
	0-%100 linear dimming

	10
	Cold white (y)
	0-255
	0-%100 linear dimming





	128 channel
	function
	Channel value
	describe

	one
	Cold white Y1
	0-255
	0-%100 linear dimming

	…
	…
	…
	…

	24
	Cold white Y24
	0-255
	0-%100 linear dimming

	25
	White W1
	0-255
	0-%100 linear dimming

	…
	…
	…
	…

	fifty-six
	White W32
	0-255
	0-%100 linear dimming

	57
	Auxiliary light R1
	0-255
	0-%100 linear dimming

	58
	Auxiliary light G1
	0-255
	0-%100 linear dimming

	59
	Auxiliary light B1
	0-255
	0-%100 linear dimming

	…
	…
	…
	…

	126
	Auxiliary light R24
	0-255
	0-%100 linear dimming

	127
	Auxiliary light G24
	0-255
	0-%100 linear dimming

	128
	Auxiliary light B24
	0-255
	0-%100 linear dimming



	10 channels
	function
	Channel value
	describe

	one
	Total dimming
	0-255
	0-%100 linear dimming

	2
	stroboscopic
	0-9
	neutrality

	
	
	10-255
	Strobe from slow to fast

	three
	Combined effect
	0
	all-or-none

	
	
	one
	R

	
	
	2
	G

	
	
	three
	B

	
	
	four
	RG

	
	
	five
	RB

	
	
	six
	GB

	
	
	seven
	RGB

	
	
	eight
	W

	
	
	nine
	Y

	
	
	10
	RGBWY

	
	
	11
	gradual change

	
	
	12
	Pulse change

	
	
	13
	jump

	
	
	14
	Effect 1

	
	
	…
	…

	
	
	250
	Effect 237

	
	
	251-255
	sound-controlled

	four
	Combined effect speed
	0-255
	Speed from slow to fast

	five
	Combination effect color selection
	0-15
	be invalid

	
	
	16-50
	R

	
	
	51-85
	G

	
	
	86-120
	B

	
	
	121-155
	RG

	
	
	156-190
	RB

	
	
	191-225
	GB

	
	
	226-255
	RGB

	six
	Red (r)
	0-255
	0-%100 linear dimming

	seven
	Green (g)
	0-255
	0-%100 linear dimming

	eight
	Blue (b)
	0-255
	0-%100 linear dimming

	nine
	White (w)
	0-255
	0-%100 linear dimming

	10
	Cold white (y)
	0-255
	0-%100 linear dimming

	11
	Cold white Y1
	0-255
	0-%100 linear dimming

	…
	…
	…
	…

	34
	Cold white Y24
	0-255
	0-%100 linear dimming

	35
	White W1
	0-255
	0-%100 linear dimming

	…
	…
	…
	…

	66
	White W32
	0-255
	0-%100 linear dimming

	67
	Auxiliary light R1
	0-255
	0-%100 linear dimming

	sixty-eight
	Auxiliary light G1
	0-255
	0-%100 linear dimming

	sixty-nine
	Auxiliary light B1
	0-255
	0-%100 linear dimming

	…
	…
	…
	…

	136
	Auxiliary light R24
	0-255
	0-%100 linear dimming

	137
	Auxiliary light G24
	0-255
	0-%100 linear dimming

	138
	Auxiliary light B24
	0-255
	0-%100 linear dimming




Fourth, the use of common functions
1, DMX512 control
Set the address code after power-on. If it is the first set, set the address code to 001. Connect the DMX512 console with a three-core signal line, and the digital display tube will stop flashing, indicating that the 512 signal has entered the lamps and lanterns, and the lamps and lanterns can be controlled. At this time, according to the channel table, the console is used to control related functions.
When there are multiple lamps, as long as the lamps at the back are connected with the lamps at the front with signal lines and the address code is set, the LED display panel will stop flashing because the lamps at the back are connected with the 512 signal, and then it can be controlled as the lamps at the front.
2. Other functions can be used as long as the related functions are pressed by the menu key (use the UP key or DOWM key to select the corresponding speed).

Fifth, the master-slave machine setting
Two or more identical lamps and lanterns are connected by 3-core signal lines. If any one of the main machines is set to voice control or gradual change, pulse change and jump, and other lamps and lanterns are set to 001 mode, the master-slave machine mode will be entered and the display screen of the slave machine will not flash (flashing means that the machine has not received the signal, so the connecting line must be checked).
Special attention: only one host can be set in a group of lamps. If there are multiple hosts, all lamps will flash without synchronization.

VI. Technical parameters:
[bookmark: OLE_LINK5]Voltage: AC100~240V 50/60HZ 180W
Power: 140W
Lamp beads: 24 3535*3W cold white lamp beads, 384 5050*0.2W RGB lamp beads and 256 5730*0.5W white lamp beads.
Control mode: DMX512, self-propelled, master-slave function. Each lamp bead can be controlled by points and zones.
Channels: CH05, CH10, CH128, CH138.
Dimming: 32bit 0~100% linear dimming
Features: dyeing+flash+code running point control light
Working temperature: -30 ~50℃
Strobe frequency: 1~30HZ
Appearance: metal, black
Connection mode: DMX512 input/output/power input/output.
IP grade: IP20
Size: weight:
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