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	Lighting Specifications
	Parameters

	Product Name
	Outdoor Waterproof Moving Head 3-in-1
	Product Model
	450 BSW IP
	Input Voltage: AC100V-240V 50/60HZ
Power Consumption: 600W
Light Source: USHIO NSLU7
Light source lifespan: 1500 hours
Diameter of Frontal Lens: 140mm
Beam angle: 2°-31°
CCT：7900K
[bookmark: _GoBack]CRI：＞70
Operating Temperature: -10-40℃
Control Mode: DMX512, Master-Slave, Auto Run, RDM
Channel: 28CH/20CH
Color: Linear CMY color mixing& Linear CMY color mixing Linear CTO Color Correction3200K-6700K
1 Color Wheel: 6 Colors
2 Color Wheel: 6 Colors
1 Static Gobo Wheel：16 gobos
1 Rotating Gobo Whee: 9 interchangeable gobos
Prism: 2 Prisms, Independent Rotation, Can be Overlapped
Frost Filter: 1 Frost Filter
Homogenizer：1 homogenizer lens
Dimming: 0-100% Smooth Dimming
Strobe: 1-20 Times/Second, Adjustable Speed
IP Rating: IP66, Waterproof
Pan scan: 540 Degrees 16 bit
Tilt scan: 270 Degrees 16 bit
Display: LCD Display with 4 Touch Buttons
Cooling Fan: Mute Fan, Variable Speed
Shell: Magnesium Alloy
Data In/Out: DMX 3-pin Input/Output + 5-pin Input/Output
Power In/Out: Waterproof power connector in/out
Product Dimensions: 709*386*290mm
Packing Dimensions:790*405*485mm
Net Weight: 27kg
Gross Weight: 30kg


	
	
	Light Color
	Black
	

	Net Weight
	27kg
	Gross Weight
	30kg
	

	Product Dimensions
	709*386*290mm
	Packing Dimensions
	790*405*485mm
	

	Protection Rating
	IP66
	Lighting Material
	All-magnesium alloy body 
	

	
	
	
	
	

	Optical System
	Effect System
	

	Light Source Information
	USHIO NSLU7
	Rotating Gobos
	1 rotating gobo wheel with 9 interchangeable gobos
	

	Light Source Life
	1500 hours
	Static Gobos
	1 Static Gobo Wheel with 16 Gobos, Variable Speed Jitter and Bidirectional Rotation
	

	Beam Angle
	2°-31°
	Color
	1、Linear CMY color mixing system and linear CTO color temperature adjustment
2、2 Color Wheels with 12 Colors
	

	Color Temperature
	7900K
	Prism
	2 Prisms（6-facet prism , 6 facet linear prism）, Bidirectional Variable Speed Rotation, Achievable Overlay Effect
	

	Dimming
	0-100% Smooth Dimming
	Fogging
	1 Independent Frost Effect, Soft and Natural Light Spot
	

	Focus
	0~100% Electronic High-Definition Focus
	Strobe
	1-20Hz Fast Strobe per Second, with Pulse Strobe, Synchronous and Asynchronous Strobe Effects
	

	Homogenizer
	1 homogenizer lens
	
	
	

	Electrical Connection
	Control System
	

	Input Voltage
	AC 100V-240V，50/60HZ
	Mechanical Movement
	Horizontal Scanning Angle 540°, Vertical Scanning Angle 270°, Automatic Return Correction and 16bit Precision Fine-Tuning Function
	

	Total Lamp Power
	600W
	Communication Design
	DMX Wired/Wireless Transmission, Convenient and Fast Software Upgrade via DMX Data Cable
	

	Signal Connection
	3-pin/5-pin Waterproof Signal Cable & Xishang Waterproof 3-pin XLR Socket
	Heat Dissipation System
	Fan Heat Dissipation Structure and Temperature Intelligent Monitoring Technology, Automatically Adjusts Heat Dissipation System to Effectively Control Lamp Temperature
	

	Power Connection
	Waterproof Power Cable Input/Output & Xishang Waterproof Power Socket
	Control Protocol
	Auto Run, Master-Slave Mode, DMX512
	

	Display Screen
	2.8-inch Display Screen with Automatic Flip Function
	Channel Mode
	 28CH/20CH
	

	Others
	
	

	Photometric Diagram
	Color: Linear CMY Mixing System, Linear CTO Color Temperature Adjustment, 2 Color Wheels with 12 Colors
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	Gobo Wheel
	Effect
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Beam Mode

Distance (m) 5 10 20 40 60 80 100
Beam Mode (1.95) °
Lux 1764000 441000 110250 27563 12250 6891 4410
Spot Diameter 0.17 0.34 0.68 1.36 2.04 2.72 34
Beam Mode 22°
Lux 22000 5500 1375 344 153 86 55
40

Spot Diameter 2.02 4.04 8.08 16 24 32
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Gobo Mode

Distance (m 5 10 20 40 60 80 100
E

Gobo Mode (3.43) °

Lux 1840000 460000 115000 28750 12778 7188 4600
Spot Diameter 0.3 0.6 12 2.4 3.6 4.79 5.99
Gobo Mode 50°

Lux 13600 3400 850 213 94 53 34
Spot Diameter 5.87 1174 22.48 46.97 70.45 93.93 11742
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