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	Lighting Specifications
	Parameters

	Product Name
	Outdoor Waterproof Moving Head Beam Light
	Product Model
	380 BEAM IP
	Input Voltage: AC100V-240V 50/60HZ
Power Consumption: 550W
Light Source: USHIO NSLU6C
Light source lifespan: 1500 hours
Diameter of Frontal Lens: 160mm
Beam angle: 1.7°
Operating Temperature: -10-40℃
Control Mode: DMX512, Master-Slave, Auto Run, RDM
Channel: 16 Channels
1 Color Wheel: 14 colors + plus open, Features half-color and linear adjustment, enabling bi-directional rainbow effects
1 Static Gobos: 13 gobos + plus open, Variable Speed Jitter and Bidirectional Rotation
Prism:  2 Prisms, Independent Rotation, Can be Overlapped
Frost Filter: 1 Frost Filter
Dimming: 0–100% linear dimming
Strobe: 1-20 Times/Second, Adjustable Speed
IP Rating: IP66, Waterproof
Pan scan: 540 Degrees 16 bit
Tilt scan: 270 Degrees 16 bit
Display: LCD Display with 4 Touch Buttons
Cooling Fan: Mute Fan, Variable Speed
Shell: Die-cast Aluminum
Data In/Out: DMX 3-pin Input/Output + 5-pin Input/Output
Power In/Out: Waterproof power connector in/out
Product Dimensions: 631*403*289mm
Packing Dimensions: 755*445*460mm
Net Weight: 25kg
Gross Weight: 28kg
With folding clamp and arm handle






	
	
	Light Color
	Black
	

	Net Weight
	25kg
	Gross Weight
	28kg
	

	Product Dimensions
	631*403*289mm
	Packing Dimensions
	755*445*460mm
	

	Protection Rating
	IP66
	Lighting Material
	All die-cast aluminum body
	

	
	
	
	
	

	Optical System
	Effect System
	

	Light Source Information
	USHIO NSLU6C
	Rotating Gobos
	None
	

	Light Source Life
	1500 hours
	Static Gobos
	1 Static Gobo Wheel with 13 Gobos, Variable Speed Jitter and Bidirectional Rotation
	

	Beam Angle
	1.7°
	Color
	1 color wheel with 14 colors plus open white, Features half-color and linear adjustment, enabling bi-directional rainbow effects
	

	Color Temperature
	/
	Prism
	[bookmark: _GoBack]2 Prisms（8-facet prism, 24-facet prism）, Bidirectional Variable Speed Rotation, Achievable Overlay Effect
	

	Dimming
	0–100% mechanical linear dimming
	Fogging
	1 Independent Frost Effect, Soft and Natural Light Spot
	

	Focus
	0~100% electronic linear high-definition Focus
	Strobe
	1-20Hz Fast Strobe per Second, with Pulse Strobe, Synchronous and Asynchronous Strobe Effects
	

	Electrical Connection
	Control System
	

	Input Voltage
	100V-240V AC，50/60HZ
	Mechanical Movement
	Horizontal Scanning Angle 540°, Vertical Scanning Angle 270°, Automatic Return Correction and 16bit Precision Fine-Tuning Function
	

	Total Lamp Power
	550W
	Communication Design
	DMX Wired/Wireless Transmission, Convenient and Fast Software Upgrade via DMX Data Cable
	

	Signal Connection
	Waterproof signal cable
	Heat Dissipation System
	Fan Heat Dissipation Structure and Temperature Intelligent Monitoring Technology, Automatically Adjusts Heat Dissipation System to Effectively Control Lamp Temperature
	

	Power Connection
	Waterproof power input & output
	Control Protocol
	Auto Run, Master-Slave Mode, DMX512
	

	Display Screen
	Fixture and lamp usage time can be queried for easy maintenance
	Channel Mode
	16CH
	

	Others
	
	

	Photometric Diagram
	1 Color Wheel: 14colors+plus open 
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	Gobo+Prisms/Frost Filters
	Effect

	1 Static Gobos：13 gobos + plus open
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