[bookmark: _GoBack]Instructions for two-eye retro matrix lamp

1、 technical parameter
Power supply: AC90～240V, 50Hz/60Hz.
Rated power: 90W
Lamp bead parameters: 2 40W COB lamp beads, 2 segments of RGB auxiliary light, and 2 circles of lamp strips (62 0.2W RGB LED).
Control mode: international DMX512, 11/19/25 channels.
Dimming mode: 0~100% ultra-smooth dimming.
Control: voice control, self-propelled, master-slave and DMX console mode.


2、 Key operation and digital tube display instructions
[image: ]
MENU: function key UP: plus key DOWN: minus key ENTER: enter key.
Digital tube display menu description
	Addr
	A001-A512
	address code

	chnd
	11/19/25 CH
	Channel selection

	STAT
	dimm
	0-255
	Total dimming

	
	stor
	0-255
	stroboscopic

	
	Gol1
	0-255
	Main light 1

	
	Gol2
	0-255
	Main light 2

	
	Red1
	0-255
	Auxiliary light red 1

	
	Gre1
	0-255
	Auxiliary light green 1

	
	Blu1
	0-255
	Auxiliary light blue 1

	
	Red2
	0-255
	Auxiliary light red 2

	
	Gre2
	0-255
	Auxiliary light green 2

	
	Blu2
	0-255
	Auxiliary light blue 2

	
	Red1
	0-255
	Lamp band red 1

	
	Gre1
	0-255
	Light band green 1

	
	Blu1
	0-255
	Lamp band blue 1

	
	Red2
	0-255
	Lamp band red 2

	
	Gre2
	0-255
	Light band green 2

	
	Blu2
	0-255
	Lamp band blue 2

	AUTO
	Au 01-10
	10 self-propelled effects

	Soud
	Su 1 / Su 2
	Se 1-15
	Voice control effect/sensitivity

	LED
	On / Off
	The screen stands by for 30 seconds and goes out.

	disp
	On / Off
	Reverse display

	Uer
	V-10
	version number




2、 DMX channel menu

DMX 11 channel table
	passage
	numerical value
	function declaration

	CH1
	000-255
	Total dimming

	CH2
	000-255
	Total stroboscopic

	CH3
	000-255
	hot light

	CH4
	000-255
	Auxiliary light red

	CH5
	000-255
	Auxiliary light green

	CH6
	000-255
	Auxiliary light blue

	CH7
	000-255
	The lamp is reddish.

	CH8
	000-255
	The light is green

	CH9
	000-255
	Lamp band blue

	CH10
	005-255
	[bookmark: OLE_LINK1]Main light/combination effect (see attached table 1 for details)

	CH11
	000-255
	[bookmark: OLE_LINK2]Main light/combined effect speed: the forward speed is adjusted by 0-127, and the reverse speed is adjusted by 128-255;




DMX19 channel table
	passage
	numerical value
	function declaration

	CH1
	000-255
	Total dimming

	CH2
	000-255
	Main light stroboscopic

	CH3
	000-255
	Main light golden yellow 1

	CH4
	000-255
	Main light golden yellow 2, (control brightness when running the main light effect)

	CH5
	005-255
	Main light/combination effect (see attached table 1 for details)

	CH6
	000-255
	Main light/combined effect speed: the forward speed is adjusted by 0-127, and the reverse speed is adjusted by 128-255;

	CH7
	000-255
	Auxiliary light/strip strobe

	CH8
	000-255
	Auxiliary light red, (control color when running auxiliary light effect)

	CH9
	000-255
	Auxiliary light green, (control color when running auxiliary light effect)

	CH10
	000-255
	Auxiliary light blue, (control color when running auxiliary light effect)

	CH11
	000-255
	Auxiliary light effect (see attached table 1 for details)

	CH12
	000-255
	Auxiliary light effect speed: the forward speed is adjusted by 0-127, and the reverse speed is adjusted by 128-255;

	CH13
	000-255
	The light band is red (control the color when running the light band effect).

	CH14
	000-255
	The light band is green (control the color when running the light band effect).

	CH15
	000-255
	The light band is blue, (control the color when running the light band effect)

	CH16
	000-255
	Effect of light strip (see attached table 1 for details)

	CH17
	000-255
	Effect speed of light strip: the forward speed is adjusted by 0-127 and the reverse speed is adjusted by 128-255;

	CH18
	000-255
	Light band effect background color

	CH19
	000-255
	Light band effect background tone light




DMX 25 channel table
	passage
	numerical value
	function declaration

	CH1
	000-255
	Total dimming

	CH2
	000-255
	Main light stroboscopic

	CH3
	000-255
	Main light golden yellow 1

	CH4
	000-255
	Main light golden yellow 2, (control brightness when running the main light effect)

	CH5
	005-255
	Main light/combination effect (see attached table 1 for details)

	CH6
	000-255
	Main light/combined effect speed: the forward speed is adjusted by 0-127, and the reverse speed is adjusted by 128-255;

	CH7
	000-255
	Auxiliary light/strip strobe

	CH8
	000-255
	Auxiliary light red 1

	CH9
	000-255
	Auxiliary light green 1

	CH10
	000-255
	Auxiliary light blue 1

	CH11
	000-255
	Auxiliary light red 2, (control color when running auxiliary light effect)

	CH12
	000-255
	Auxiliary light green 2, (control color when running auxiliary light effect)

	CH13
	000-255
	Auxiliary light blue 2, (control color when running auxiliary light effect)

	CH14
	000-255
	Auxiliary light effect (see attached table 1 for details)

	CH15
	000-255
	Auxiliary light effect speed: the forward speed is adjusted by 0-127, and the reverse speed is adjusted by 128-255;

	CH16
	000-255
	Light with red 1

	CH17
	000-255
	Light band green 1

	CH18
	000-255
	Light band blue 1

	CH19
	000-255
	The light band is red 2, (control the color when running the light band effect)

	CH20
	000-255
	The light band is green 2, (control the color when running the light band effect)

	CH21
	000-255
	The light band is blue 2, (control the color when running the light band effect)

	CH22
	000-255
	Effect of light strip (see attached table 1 for details)

	CH23
	000-255
	Effect speed of light strip: the forward speed is adjusted by 0-127 and the reverse speed is adjusted by 128-255;

	CH24
	000-255
	Light band effect background color

	CH25
	000-255
	Light band effect background tone light





Schedule 1: Description of built-in effects and functions
	CH value
	
	CH value
	
	CH value
	

	0 - 4
	all-or-none
	0 - 4
	all-or-none
	0
	all-or-none

	5 - 16
17 - 28
29 - 40
41 - 52
53 - 64
65 - 76
77 - 88
89 - 100
101 - 112
113 - 124
125 - 136
137 - 148
149 - 160
161 - 172
173 - 184
185 - 196
197 - 208
209 - 220
221 - 232
233 - 249
	Main light effect
1 Main light effect
2 main light effect
3 main light effect
4 main light effect
5 main light effect
6 main light effect
7 main light effect
8 Main light effect 9
Main light effect cycle 10
Combined effect 1
Combined effect 2
Combined effect 3
Combined effect 4
Combined effect 5
Combined effect 6
Combined effect 7
Combined effect 8
Combined effect 9
Combined effect 10
	5 - 16
17 - 28
29 - 40
41 - 52
53 - 64
65 - 76
77 - 88
89 - 100
101 - 112
113 - 124
125 - 136
137 - 148
149 - 160
161 - 172
173 - 255

	Auxiliary light effect
1 auxiliary light effect
2 auxiliary light effect
3 auxiliary light effect
4 auxiliary light effect
5 auxiliary light effect
6 auxiliary light effect
7 auxiliary light effect
8 auxiliary light effect
9 auxiliary light effect
10 auxiliary light effect
11 auxiliary light effect
12 auxiliary light effect
13 Auxiliary light effect 14
Auxiliary light effect cycle 15
	1 - 4
5 - 8
9 - 12
13 - 16
17 - 20
21 - 24
25 - 28
29 - 32
33 - 36
37 - 40
...
217 - 220
221 - 224
225 - 228
229 - 232
233 - 236
237 - 240
241 - 244
245 - 248
249 - 252
253 - 255
	Lamp strip effect
1 light strip effect
2 light strip effect
3 light strip effect
4 light strip effect
5 light strip effect
6 light strip effect
7 light strip effect
8 light strip effect
9 light strip effect
10 ...
Light strip effect 55
Light strip effect 56
Light strip effect 57
Light strip effect 58
Light strip effect 59
Lamp Strip Effect 60
Light strip effect 61
Light strip effect 62
Light strip effect 63
Light Strip Effect Cycle 64


	250 - 252
	Voice control effect 1
	
	
	
	

	253 - 255
	Voice control effect 2
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