Instructions for four-eye retro matrix lamp
1、 technical parameter
Power supply: AC90～240V, 50Hz/60Hz.
Rated power: 180W
Lamp bead parameters: 4 40W COB lamp beads, 4 segments of RGB auxiliary light, and 4 circles of lamp strips (124 0.2W RGB LED).
Control mode: international DMX512, 11/23/32 channel.
Dimming mode: 0~100% ultra-smooth dimming.
Control: voice control, self-propelled, master-slave and DMX console mode.


2、 Key operation and digital tube display instructions
[image: ]
MENU: function key	UP: DOWN: ENTER: Enter: Enter.
Digital tube display menu description
	Address
	A001-A512
	address code

	Channel
	11/23/32 CH
	Channel selection

	STAT
	dimm
	000-255
	Total dimming

	
	stor
	000-255
	Main light stroboscopic

	
	Gol1
	000-255
	Main light golden yellow 1

	
	Gol2
	000-255
	Main light golden yellow 2

	
	Gol3
	000-255
	Main light golden yellow 3

	
	Gol4
	000-255
	Main light golden yellow 4
(Control the brightness when running the main light effect)

	
	efet
	005-255
	Main light/combination effect

	
	sped
	000-255
	Main light/combined effect speed: the forward speed is adjusted by 0-127, and the reverse speed is adjusted by 128-255;

	
	stor
	000-255
	Auxiliary light/strip strobe

	
	Red
	000-255
	Auxiliary light red
(Control the color when running the auxiliary light effect)

	
	Gre
	000-255
	Auxiliary light green
(Control the color when running the auxiliary light effect)

	
	Blu
	000-255
	Auxiliary light blue
(Control the color when running the auxiliary light effect)

	
	efet
	000-255
	Auxiliary light effect

	
	sped
	000-255
	Auxiliary light effect speed: the forward speed is adjusted by 0-127, and the reverse speed is adjusted by 128-255;

	
	bgcl
	000-255
	Auxiliary light effect background color

	
	bgdi
	000-255
	Auxiliary light effect background tone light

	
	Red
	000-255
	The light is reddish.
(Control the color when running the light strip effect)

	
	Gre
	000-255
	The light is green.
(Control the color when running the light strip effect)

	
	Blu
	000-255
	The light is blue.
(Control the color when running the light strip effect)

	
	efet
	000-255
	Lamp strip effect

	
	sped
	000-255
	Effect speed of light strip: the forward speed is adjusted by 0-127 and the reverse speed is adjusted by 128-255;

	
	bgcl
	000-255
	Light band effect background color

	
	bgdi
	000-255
	Light band effect background tone light

	AUTO
	Au 1-10
	Speed  1-15
	10 self-propelled effects

	Soud
	Su 1-2
	Sensitivity  1-15
	Voice control effect/sensitivity

	LED
	On / Off
	The screen stands by for 30 seconds and goes out.

	disp
	On / Off
	Reverse display

	Uer
	V-11
	version number



2、 DMX channel menu

DMX 11 channel table
	passage
	numerical value
	function declaration

	CH1
	000-255
	Total dimming

	CH2
	000-255
	Total stroboscopic

	CH3
	000-255
	hot light

	CH4
	000-255
	Auxiliary light red

	CH5
	000-255
	Auxiliary light green

	CH6
	000-255
	Auxiliary light blue

	CH7
	000-255
	The lamp is reddish.

	CH8
	000-255
	The light is green

	CH9
	000-255
	Lamp band blue

	CH10
	005-255
	[bookmark: OLE_LINK1]Main light/combination effect (see attached table 1 for details)

	CH11
	000-255
	Main light/combined effect speed: the forward speed is adjusted by 0-127, and the reverse speed is adjusted by 128-255;




DMX 23 channel table
	passage
	numerical value
	function declaration

	CH1
	000-255
	Total dimming

	CH2
	000-255
	Main light stroboscopic

	CH3
	000-255
	Main light golden yellow 1

	CH4
	000-255
	Main light golden yellow 2

	CH5
	000-255
	Main light golden yellow 3

	CH6
	000-255
	Main light golden yellow 4, (control brightness when running the main light effect)

	CH7
	005-255
	Main light/combination effect (see attached table 1 for details)

	CH8
	000-255
	Main light/combined effect speed: the forward speed is adjusted by 0-127, and the reverse speed is adjusted by 128-255;

	CH9
	000-255
	Auxiliary light/strip strobe

	CH10
	000-255
	Auxiliary light red, (control color when running auxiliary light effect)

	CH11
	000-255
	Auxiliary light green, (control color when running auxiliary light effect)

	CH12
	000-255
	Auxiliary light blue, (control color when running auxiliary light effect)

	CH13
	000-255
	Auxiliary light effect (see attached table 1 for details)

	CH14
	000-255
	Auxiliary light effect speed: the forward speed is adjusted by 0-127, and the reverse speed is adjusted by 128-255;

	CH15
	000-255
	Auxiliary light effect background color

	CH16
	000-255
	Auxiliary light effect background tone light

	CH17
	000-255
	The light band is red (control the color when running the light band effect).

	CH18
	000-255
	The light band is green (control the color when running the light band effect).

	CH19
	000-255
	The light band is blue, (control the color when running the light band effect)

	CH20
	000-255
	Effect of light strip (see attached table 1 for details)

	CH21
	000-255
	Effect speed of light strip: the forward speed is adjusted by 0-127 and the reverse speed is adjusted by 128-255;

	CH22
	000-255
	Light band effect background color

	CH23
	000-255
	Light band effect background tone light




DMX 32 channel table
	passage
	numerical value
	function declaration

	CH1
	000-255
	Total dimming

	CH2
	000-255
	Main light stroboscopic

	CH3
	000-255
	Main light golden yellow 1

	CH4
	000-255
	Main light golden yellow 2

	CH5
	000-255
	Main light golden yellow 3

	CH6
	000-255
	Main light golden yellow 4, (control brightness when running the main light effect)

	CH7
	005-255
	Main light/combination effect (see attached table 1 for details)

	CH8
	000-255
	Main light/combined effect speed: the forward speed is adjusted by 0-127, and the reverse speed is adjusted by 128-255;

	CH9
	000-255
	Auxiliary light/strip strobe

	CH10
	000-255
	Auxiliary light red 1

	CH11
	000-255
	Auxiliary light green 1

	CH12
	000-255
	Auxiliary light blue 1

	...
	...
	...

	...
	...
	...

	CH19
	000-255
	Auxiliary light red 4, (control color when running auxiliary light effect)

	CH20
	000-255
	Auxiliary light green 4, (control color when running auxiliary light effect)

	CH21
	000-255
	Auxiliary light blue 4, (control color when running auxiliary light effect)

	CH22
	000-255
	Auxiliary light effect (see attached table 1 for details)

	CH23
	000-255
	Auxiliary light effect speed: the forward speed is adjusted by 0-127, and the reverse speed is adjusted by 128-255;

	CH24
	000-255
	Auxiliary light effect background color

	CH25
	000-255
	Auxiliary light effect background tone light

	CH26
	000-255
	The light band is red (control the color when running the light band effect).

	CH27
	000-255
	The light band is green (control the color when running the light band effect).

	CH28
	000-255
	The light band is blue, (control the color when running the light band effect)

	CH29
	000-255
	Effect of light strip (see attached table 1 for details)

	CH30
	000-255
	Effect speed of light strip: the forward speed is adjusted by 0-127 and the reverse speed is adjusted by 128-255;

	CH31
	000-255
	Light band effect background color

	CH32
	000-255
	Light band effect background tone light






Schedule 1: Description of built-in effects and functions
	CH value
	
	CH value
	
	CH value
	

	0 - 4
	all-or-none
	0 - 4
	all-or-none
	0
	all-or-none

	5 - 12
13 - 20
21 - 28
29 - 36
37 - 44
45 - 52
53 - 60
61 - 68
69 - 76
77 - 84
85 - 92
93 - 100
101 - 108
109 - 116
117 - 124
125 - 132
133 - 140
141 - 148
149 - 156
157 - 164
165 - 172
173 - 180
181 - 188
189 - 196
197 - 204
205 - 212
213 - 220
221 - 228
229 - 236
237 - 249
	Main light effect 1
Main light effect 2
Main light effect 3
Main light effect 4
Main light effect 5
Main light effect 6
Main light effect 7
Main light effect 8
Main light effect 9
Main light effect 10
Main light effect 11
Main light effect 12
Main light effect 13
Main light effect 14
Main light effect 15
Main light effect 16
Main light effect 17
Main light effect 18
Main light effect 19
Main light effect cycle 20
Combined effect 1
Combined effect 2
Combined effect 3
Combined effect 4
Combined effect 5
Combined effect 6
Combined effect 7
Combined effect 8
Combined effect 9
Combined effect 10
	5 - 12
13 - 20
21 - 28
29 - 36
37 - 44
45 - 52
53 - 60
61 - 68
69 - 76
77 - 84
85 - 92
93 - 100
101 - 108
109 - 116
117 - 124
125 - 132
133 - 140
141 - 148
149 - 156
157 - 164
165 - 172
173 - 180
181 - 188
189 - 196
197 - 204
205 - 212
213 - 220
221 - 228
229 - 236
237 - 255
	Auxiliary light effect 1
Auxiliary light effect 2
Auxiliary light effect 3
Auxiliary light effect 4
Auxiliary light effect 5
Auxiliary light effect 6
Auxiliary light effect 7
Auxiliary light effect 8
Auxiliary light effect 9
Auxiliary light effect 10
Auxiliary light effect 11
Auxiliary light effect 12
Auxiliary light effect 13
Auxiliary light effect 14
Auxiliary light effect 15
Auxiliary light effect 16
Auxiliary light effect 17
Auxiliary light effect 18
Auxiliary light effect 19
Auxiliary light effect 20
Auxiliary light effect 21
Auxiliary light effect 22
Auxiliary light effect 23
Auxiliary light effect 24
Auxiliary light effect 25
Auxiliary light effect 26
Auxiliary light effect 27
Auxiliary light effect 28
Auxiliary light effect 29
Auxiliary light effect cycle 30
	1 - 3
4 - 6
7 - 9
10 - 12
13 - 15
16 - 18
19 - 21
22 - 24
25 - 27
28 - 30
31 - 33
34 - 36
37 - 39
40 - 42
...
211 - 213
214 - 216
217 - 219
220 - 222
223 - 225
226 - 228
229 - 231
232 - 234
235 - 237
238 - 240
241 - 243
244 - 246
247 - 249
250 - 252
253 - 255
	Lamp strip effect 1
Lamp strip effect 2
Lamp strip effect 3
Light strip effect 4
Light strip effect 5
Lamp strip effect 6
Light strip effect 7
Light strip effect 8
Lamp strip effect 9
Light Strip Effect 10
Light Strip Effect 11
Lamp Strip Effect 12
Lamp Strip Effect 13
Light Strip Effect 14
[bookmark: OLE_LINK2]...
Light strip effect 71
Light strip effect 72
Light strip effect 73
Light strip effect 74
Light strip effect 75
Light strip effect 76
Light strip effect 77
Light strip effect 78
Light strip effect 79
Light strip effect 80
Light strip effect 81
Light strip effect 82
Light strip effect 83
Light strip effect 84
Light Strip Effect Cycle 85


	250 - 252
	Voice control effect 1
	
	
	
	

	253 - 255
	Voice control effect 2
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